| back |  | Last regenerated: 2022-04-20 17:31:36 kio

# zasm - Z80 Assembler – Version 4.4

# Targets

[<prev] [next>]

| ### #target TZX #### 0x13: Sequence of pulses of various lengths
    #tzx PULSES
        Pseudo instructions: defw, dw, .dw, .word
    8080 pseudo instructions: DWdw  NN, ...
This block stores up to 255 individual pulses. It can be used to create custom sync pulses after block 0x12 with a custom pilot tone. The pulse length is based on ZX Spectrum clock cycles. (3.5MHz) |

[<prev] [top] [next>]