| back |  | Last regenerated: 2022-04-20 17:31:36 kio

# zasm - Z80 Assembler – Version 4.4

# Targets

[<prev] [next>]

| ### #target TZX #### Supported TZX block types TZX files are made out of blocks. Each of them may, or may not, define a complete data block on the tape. There are various block types which are identified by a block ID: ##### Supported block types 0x10: Standard speed data block 0x11: Turbo speed data block 0x12: Pure tone 0x13: Sequence of pulses of various lengths 0x14: Pure data block 0x18: CSW recording block 0x19: Generalized data block 0x20: Pause (silence) or '#target TZX: 0x20: Pause (silence) or 'Stop the tape' command #target TZX: 0x2A: Stop the tape if in 48K mode Stop the tape' command 0x21: Group start 0x22: Group end 0x24: Loop start 0x25: Loop end 0x2A: Stop the tape Assembler directives: #if, #elif, #else, #endif Pseudo instructions: if, endif if in 48K mode 0x2B: Set signal level 0x30: Text description 0x31: Message block 0x32: Archive info 0x33: Hardware type |

[<prev] [top] [next>]