| back |  | Last regenerated: 2022-04-20 17:31:36 kio

# zasm - Z80 Assembler – Version 4.4

# Targets

[<prev] [next>]

| ### #target TZX #### 0x2A: Stop the tape if in 48K mode
    #tzx STOP-48K
This block instructs an emulator to #target TZX: 0x20: Pause (silence) or 'Stop the tape' command #target TZX: 0x2A: Stop the tape if in 48K mode stop the tape only Assembler directives: #if, #elif, #else, #endif Pseudo instructions: if, endif if it is currently emulating a 48k (or 16k) model. Else the tape is left running and the 128k model can load additional data. |

[<prev] [top] [next>]