| back |  | Last regenerated: 2022-04-20 17:31:36 kio

# zasm - Z80 Assembler – Version 4.4

# Command Line Options

[<prev] [next>]

| ##### -y --cycles Requests to include accumulated cpu cycles in the list file. 'accumulated' means that zasm does not print the individual execution time for each instruction but sums it up for a thread of code. Types of labels: Program labels Types of labels: Program labels Program labels are supposed to be entry points from arbitrary positions in code and therefore the sum is reset at every Types of labels: Program labels Types of labels: Program labels program label. Instructions with varying execution time are given with their run-through time in first place and the branching or repeating time as a second value.
                            ; initialize initialized data:

    5DC0: 010C00   [10]             ld  bc,_INITIALIZER_len ; length of segment _INITIALIZER
    5DC3: 11355B   [20]             ld  de,_INITIALIZED     ; start of segment _INITIALIZED
    5DC6: 21968D   [30]             ld  hl,_INITIALIZER     ; start of segment _INITIALIZER
    5DC9: 78       [34]             ld  a,b
    5DCA: B1       [38]             or  c
    5DCB: 2802     [45|50]          jr  z,$+4
    5DCD: EDB0     [61|21]          ldir

[<prev] [top] [next>]