| back |  | Last regenerated: 2022-04-20 17:31:36 kio

# zasm - Z80 Assembler – Version 4.4

# Command Line Options

[<prev] [next>]

| ##### -x --hex Request to write the output file in Intel Hex format. This is only allowed for target ROM (the default) or target BIN.
    :200000003E00ED79ED79ED793E40ED793EDAED793E37ED79ED780F30FB3A1027D370ED787B
    :090020000F0F30FADB70321027DB
    :00000001FF

[<prev] [top] [next>]