| back |  | Last regenerated: 2022-04-20 17:31:36 kio

# zasm - Z80 Assembler – Version 4.4

# Targets

[<prev] [next>]

| ### #target TZX #### 0x20: Pause (silence) or 'Stop the tape' command
    #tzx PAUSE, [DURATION=]pause
Insert silence into the tape. DURATION: duration in ms. Assembler directives: #if, #elif, #else, #endif Pseudo instructions: if, endif If PAUSE=0 then an emulator will #target TZX: 0x20: Pause (silence) or 'Stop the tape' command #target TZX: 0x2A: Stop the tape if in 48K mode stop the tape. |

[<prev] [top] [next>]