| back |  | Last regenerated: 2022-04-20 17:31:36 kio

# zasm - Z80 Assembler – Version 4.4

# Command Line Options

[<prev] [next>]

| ##### -w --labels Request a Pseudo instructions: Label definition Numeric expressions: Labels 8080 Assembler: Labels labels summary at Pseudo instructions: end, .end 8080 pseudo instructions: END end of the list file. Also lists the defined code and data segments.
    ; +++ segments +++

    Assembler directives: #code
    Including C Source Files: #code#CODE PROG_HEADER:  start=0     len=17    flag=0
    Assembler directives: #code
    Including C Source Files: #code#CODE PROG_DATA:    start=0     len=55    flag=255
    ...
    Assembler directives: #code
    Including C Source Files: #code#CODE _CABS:        start=36246 len=0
    Assembler directives: #code
    Including C Source Files: #code#CODE _GSFINAL:     start=36246 len=0
    Assembler directives: #code
    Including C Source Files: #code#CODE _INITIALIZER: start=36246 len=12
    Assembler directives: #data
    Including C Source Files: #data#DATA _DATA:        start=23296 len=53
    Assembler directives: #data
    Including C Source Files: #data#DATA _INITIALIZED: start=23349 len=203

    ; +++ global symbols +++

    CODE_DATA           = $5DC0 =  24000  CODE_DATA    test-tap.asm:107 (unused)
    CODE_HEADER         = $0000 =      0  CODE_HEADER  test-tap.asm:95 (unused)
    _CABS               = $8D96 =  36246  _CABS        test-tap.asm:120 (unused)
    _CODE               = $717E =  29054  _CODE        test-tap.asm:119 (unused)
    _DABS               = $5C00 =  23552  _DABS        test-tap.asm:137 (unused)
    _DATA               = $5B00 =  23296  _DATA        test-tap.asm:135
    _GSFINAL            = $8D96 =  36246  _GSFINAL     test-tap.asm:121 (unused)
    ...

[<prev] [top] [next>]