| back |  | Last regenerated: 2022-04-20 17:31:36 kio

# zasm - Z80 Assembler – Version 4.4

# Command Line Options

[<prev] [next>]

| ##### -s --s19 Request to write the output file in Motorola S-Record format. This is only allowed for target ROM (the default) or target BIN. This format supports a header and zasm uses it to store the source file name and assembly date. Since it is encoded as hex data, it is not directly readable in the #insert: Examples: #assert: Example: incbin: Examples: #assert: Example:example below:
    S00F00007320323031352D30312D313178
    S12C00003E00ED79ED79ED793E40ED793EDAED793E37ED79ED780F30FB3A1027D370ED780F0F30FADB7032102772
    S5030001FB
    S9030000FC

[<prev] [top] [next>]