| back |  | Last regenerated: 2022-04-20 17:31:36 kio

# zasm - Z80 Assembler – Version 4.4

# Targets

[<prev] [next>]

| ### #target TZX #### 0x2B: Set signal level
    #tzx POLARITY, [POLARITY=]polarity
Pseudo instructions: defl, set and '=' Labels: SET Set the signal polarity. The ZX Spectrum tape loading routines are polarity insensitive but e.g. the ZX81 routines weren't. This block can be used to force the polarity of the following pulses. POLARITY: 0=low, 1=high. |

[<prev] [top] [next>]