<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 09:47:05</description>
<packages>
<package name="SOIC127P600X175-8N">
</package>
<package name="SOIC127P1030X265-16N">
</package>
<package name="SOIC127P600X175-14N">
</package>
<package name="SOIC127P600X175-16N">
</package>
<package name="DIP254P762X533-8">
</package>
<package name="DIP254P762X533-14">
</package>
<package name="SOIC127P1032X265-16N">
</package>
<package name="DIP254P1524X635-28">
</package>
<package name="SOIC127PX1032X265-28N">
</package>
<package name="SOT95P240X112-3N">
</package>
<package name="SOT95P237X112-3N">
</package>
<package name="DIP254P762X533-16">
</package>
</packages>
<symbols>
<symbol name="AUIR2085S">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="AUIRF7343Q">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="G1" direction="pas"/>
<pin name="G2" direction="pas"/>
<pin name="D1_2" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2_2" direction="pas"/>
<pin name="D2" direction="pas"/>
</symbol>
<symbol name="AUIRS2004S">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="AUIRS2016S">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="RESET-" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS2110S">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS2112S">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="SD" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS2113S">
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS2117S">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS2118S">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS21271S">
<pin name="VCC" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="VS" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS2127S">
<pin name="VCC" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="VS" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS21281S">
<pin name="VCC" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="VS" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS2128S">
<pin name="VCC" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="~IN" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="VS" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS21811S">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="AUIRS21814S">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="AUIRS2181S">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="AUIRS21844S">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="IN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="DT" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="AUIRS2184S">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="AUIRS2191S">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC_6" direction="nc"/>
<pin name="NC_7" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS2301S">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS2302S">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="AUIRS4426S">
<pin name="VS" direction="pwr"/>
<pin name="~INA" direction="in"/>
<pin name="~INB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="AUIRS4428S">
<pin name="VS" direction="pwr"/>
<pin name="~INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="IR1150IPBF">
<pin name="VCC" direction="pwr"/>
<pin name="FREQ" direction="in"/>
<pin name="ISNS" direction="in"/>
<pin name="OVP/EN" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="VFB" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="IR1150ISTRPBF">
<pin name="VCC" direction="pwr"/>
<pin name="COMP" direction="in"/>
<pin name="VFB" direction="in"/>
<pin name="ISNS" direction="in"/>
<pin name="OVP/EN" direction="in"/>
<pin name="FREQ" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="GATE" direction="out"/>
</symbol>
<symbol name="IR11662SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VD" direction="in"/>
<pin name="VS" direction="in"/>
<pin name="OVT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="MOT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VGATE" direction="out"/>
</symbol>
<symbol name="IR11672ASPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VD" direction="in"/>
<pin name="VS" direction="in"/>
<pin name="MOT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="OVT" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VGATE" direction="out"/>
</symbol>
<symbol name="IR11682SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VD1" direction="in"/>
<pin name="VD2" direction="in"/>
<pin name="VS1" direction="in"/>
<pin name="VS2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GATE1" direction="out"/>
<pin name="GATE2" direction="out"/>
</symbol>
<symbol name="IR1168SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS1" direction="in"/>
<pin name="VS2" direction="in"/>
<pin name="VD1" direction="in"/>
<pin name="VD2" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="GATE1" direction="out"/>
<pin name="GATE2" direction="out"/>
</symbol>
<symbol name="IR2010PBF">
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="SD" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2010SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="VS" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2011PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2101PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2102SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="~LIN" direction="in"/>
<pin name="~HIN" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2103SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="~LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2104PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2104STRPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2106SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR21084SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pas"/>
<pin name="~LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="DT" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2108PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="~LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2108SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="~LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2110-1PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="SD" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2110-2PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="VB" direction="pas"/>
<pin name="SD" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2110PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="SD" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2110SPBF">
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2110STRPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="VS" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2111PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2111SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2111STRPBF">
<pin name="VCC" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="VB" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2112PBF">
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="SD" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2112SPBF">
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2113PBF">
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="SD" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2113SPBF">
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2113STRPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="VS" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2117PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2117SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="VB" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2118PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="~IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2118STRPBF">
<pin name="VCC" direction="pwr"/>
<pin name="~IN" direction="in"/>
<pin name="VB" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2121PBF">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="ERR" direction="in"/>
<pin name="CS" direction="pas"/>
<pin name="IN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="IR2125PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="ERR" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR21271SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="VB" direction="pwr"/>
<pin name="CS" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="~FAULT" direction="out"/>
</symbol>
<symbol name="IR2127PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="CS" direction="pas"/>
<pin name="IN" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2130PBF">
<pin name="VCC" direction="pwr"/>
<pin name="CA-" direction="in"/>
<pin name="CA0" direction="in"/>
<pin name="VB1" direction="pwr"/>
<pin name="VB2" direction="in"/>
<pin name="VB3" direction="in"/>
<pin name="VS0" direction="in"/>
<pin name="VS1" direction="pwr"/>
<pin name="VS2" direction="pwr"/>
<pin name="VS3" direction="pwr"/>
<pin name="ITRIP" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="~LIN1" direction="in"/>
<pin name="~LIN2" direction="in"/>
<pin name="~LIN3" direction="in"/>
<pin name="~HIN1" direction="in"/>
<pin name="~HIN2" direction="in"/>
<pin name="~HIN3" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO1" direction="out"/>
<pin name="LO2" direction="out"/>
<pin name="LO3" direction="out"/>
<pin name="HO1" direction="out"/>
<pin name="HO2" direction="out"/>
<pin name="HO3" direction="out"/>
</symbol>
<symbol name="IR2130SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="CA-" direction="in"/>
<pin name="ITRIP" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="CAO" direction="in"/>
<pin name="VSO" direction="in"/>
<pin name="~HIN1" direction="in"/>
<pin name="~HIN2" direction="in"/>
<pin name="~HIN3" direction="in"/>
<pin name="~LIN1" direction="in"/>
<pin name="~LIN2" direction="in"/>
<pin name="~LIN3" direction="in"/>
<pin name="VB1" direction="in"/>
<pin name="VB2" direction="in"/>
<pin name="VB3" direction="out"/>
<pin name="VS1" direction="in"/>
<pin name="VS2" direction="out"/>
<pin name="VS3" direction="out"/>
<pin name="VSS" direction="pas"/>
<pin name="LO1" direction="out"/>
<pin name="LO2" direction="out"/>
<pin name="LO3" direction="out"/>
<pin name="HO1" direction="out"/>
<pin name="HO2" direction="out"/>
<pin name="HO3" direction="out"/>
</symbol>
<symbol name="IR2131SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="SD" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="ITRIP" direction="in"/>
<pin name="~FLT-CLR" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="~HIN1" direction="in"/>
<pin name="~HIN2" direction="in"/>
<pin name="~HIN3" direction="in"/>
<pin name="~LIN1" direction="in"/>
<pin name="~LIN2" direction="in"/>
<pin name="~LIN3" direction="in"/>
<pin name="VB1" direction="in"/>
<pin name="VB2" direction="in"/>
<pin name="VB3" direction="out"/>
<pin name="VS1" direction="in"/>
<pin name="VS2" direction="out"/>
<pin name="VS3" direction="out"/>
<pin name="VSS" direction="pas"/>
<pin name="LO1" direction="out"/>
<pin name="LO2" direction="out"/>
<pin name="LO3" direction="out"/>
<pin name="HO1" direction="out"/>
<pin name="HO2" direction="out"/>
<pin name="HO3" direction="out"/>
</symbol>
<symbol name="IR2132SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="CA-" direction="in"/>
<pin name="ITRIP" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="CAO" direction="in"/>
<pin name="VSO" direction="in"/>
<pin name="~HIN1" direction="in"/>
<pin name="~HIN2" direction="in"/>
<pin name="~HIN3" direction="in"/>
<pin name="~LIN1" direction="in"/>
<pin name="~LIN2" direction="in"/>
<pin name="~LIN3" direction="in"/>
<pin name="VB1" direction="in"/>
<pin name="VB2" direction="in"/>
<pin name="VB3" direction="out"/>
<pin name="VS1" direction="in"/>
<pin name="VS2" direction="out"/>
<pin name="VS3" direction="out"/>
<pin name="VSS" direction="pas"/>
<pin name="LO1" direction="out"/>
<pin name="LO2" direction="out"/>
<pin name="LO3" direction="out"/>
<pin name="HO1" direction="out"/>
<pin name="HO2" direction="out"/>
<pin name="HO3" direction="out"/>
</symbol>
<symbol name="IR21362PBF">
<pin name="VCC" direction="pwr"/>
<pin name="ITRIP" direction="in"/>
<pin name="RCIN" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="VB1" direction="pwr"/>
<pin name="VB2" direction="in"/>
<pin name="VB3" direction="in"/>
<pin name="VS1" direction="pwr"/>
<pin name="VS2" direction="pwr"/>
<pin name="VS3" direction="pwr"/>
<pin name="~LIN1" direction="in"/>
<pin name="~LIN2" direction="in"/>
<pin name="~LIN3" direction="in"/>
<pin name="HIN1" direction="in"/>
<pin name="HIN2" direction="in"/>
<pin name="HIN3" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO1" direction="out"/>
<pin name="LO2" direction="out"/>
<pin name="LO3" direction="out"/>
<pin name="HO1" direction="out"/>
<pin name="HO2" direction="out"/>
<pin name="HO3" direction="out"/>
</symbol>
<symbol name="IR2136SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="RCIN" direction="in"/>
<pin name="~FAULT" direction="in"/>
<pin name="ITRIP" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="HIN1" direction="in"/>
<pin name="HIN2" direction="in"/>
<pin name="HIN3" direction="in"/>
<pin name="~LIN1" direction="in"/>
<pin name="~LIN2" direction="in"/>
<pin name="~LIN3" direction="in"/>
<pin name="VB1" direction="in"/>
<pin name="VB2" direction="in"/>
<pin name="VB3" direction="out"/>
<pin name="VS1" direction="in"/>
<pin name="VS2" direction="out"/>
<pin name="VS3" direction="out"/>
<pin name="VSS" direction="pas"/>
<pin name="LO1" direction="out"/>
<pin name="LO2" direction="out"/>
<pin name="LO3" direction="out"/>
<pin name="HO1" direction="out"/>
<pin name="HO2" direction="out"/>
<pin name="HO3" direction="out"/>
</symbol>
<symbol name="IR21531DPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="CT" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2153DPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="RT" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2153PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="RT" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR21834STRPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pas"/>
<pin name="DT" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="HIN" direction="in"/>
<pin name="~LIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="VS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2183PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="~LIN" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR21844SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="IN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="DT" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2184PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="~SD" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IR2213PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="SD" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR2213SPBF">
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IR4426PBF">
<pin name="VS" direction="pwr"/>
<pin name="~INA" direction="in"/>
<pin name="~INB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="IR4427PBF">
<pin name="VS" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="IR4427SPBF">
<pin name="VS" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="IR4428PBF">
<pin name="VS" direction="pwr"/>
<pin name="~INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
</symbol>
<symbol name="IRF7815PBF">
<pin name="S_2" direction="pas"/>
<pin name="S_3" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D_2" direction="pas"/>
<pin name="D_3" direction="pas"/>
<pin name="D_4" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="IRF9332PBF">
<pin name="S_2" direction="pas"/>
<pin name="S_3" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D_2" direction="pas"/>
<pin name="D_3" direction="pas"/>
<pin name="D_4" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="IRF9358PBF">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="G1" direction="pas"/>
<pin name="G2" direction="pas"/>
<pin name="D1_2" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2_2" direction="pas"/>
<pin name="D2" direction="pas"/>
</symbol>
<symbol name="IRF9362PBF">
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="G1" direction="pas"/>
<pin name="G2" direction="pas"/>
<pin name="D1_2" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2_2" direction="pas"/>
<pin name="D2" direction="pas"/>
</symbol>
<symbol name="IRFML8244TRPBF">
<pin name="G" direction="in"/>
<pin name="S" direction="pas"/>
<pin name="D" direction="out"/>
</symbol>
<symbol name="IRL6342PBF">
<pin name="S_2" direction="pas"/>
<pin name="S_3" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D_2" direction="pas"/>
<pin name="D_3" direction="pas"/>
<pin name="D_4" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="IRLML2244TRPBF">
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="IRLML2246TRPBF">
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="IRLML6244TRPBF">
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="IRLML6246TRPBF">
<pin name="G" direction="in"/>
<pin name="S" direction="pas"/>
<pin name="D" direction="out"/>
</symbol>
<symbol name="IRLML6344TRPBF">
<pin name="G" direction="in"/>
<pin name="S" direction="pas"/>
<pin name="D" direction="out"/>
</symbol>
<symbol name="IRLML6346TRPBF">
<pin name="G" direction="in"/>
<pin name="S" direction="pas"/>
<pin name="D" direction="out"/>
</symbol>
<symbol name="IRS2001SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IRS2003PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="~LIN" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS2003SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="~LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IRS2011SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IRS20124SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pas"/>
<pin name="DT/SD" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="OCSET1" direction="in"/>
<pin name="OCSET2" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
<pin name="~OC" direction="out"/>
</symbol>
<symbol name="IRS2092PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="pwr"/>
<pin name="OCSET" direction="pas"/>
<pin name="VS" direction="in"/>
<pin name="VB" direction="pas"/>
<pin name="VAA" direction="pwr"/>
<pin name="DT" direction="in"/>
<pin name="CSH" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="CSD" direction="pas"/>
<pin name="COMP_2" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS20957SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VREF" direction="pas"/>
<pin name="IN" direction="in"/>
<pin name="DT" direction="in"/>
<pin name="OCSET" direction="pas"/>
<pin name="CSH" direction="in"/>
<pin name="CSD" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS2153DPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="RT" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS21844PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="~SD" direction="in"/>
<pin name="DT" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="IN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS21851SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="in"/>
<pin name="VS" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pas"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS21864PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="LIN" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS21864SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="HIN" direction="in"/>
<pin name="~LIN" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC_5" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IRS2186PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="~LIN" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS2186STRPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="HIN" direction="in"/>
<pin name="LIN" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS21952SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="LIN1" direction="in"/>
<pin name="LIN2" direction="in"/>
<pin name="HIN" direction="in"/>
<pin name="COM" direction="pwr"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC_4" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pas"/>
<pin name="LO1" direction="out"/>
<pin name="LO2" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS2541PBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="ENN" direction="in"/>
<pin name="IFB" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS2552DPBF">
<pin name="VCC" direction="pwr"/>
<pin name="COM" direction="pas"/>
<pin name="DIM" direction="in"/>
<pin name="MIN" direction="in"/>
<pin name="MAX" direction="in"/>
<pin name="CT" direction="pas"/>
<pin name="ENA" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="SD" direction="out"/>
<pin name="CS" direction="in"/>
<pin name="CD" direction="in"/>
<pin name="DT" direction="pas"/>
<pin name="VB" direction="pas"/>
<pin name="VS" direction="pwr"/>
<pin name="HO" direction="out"/>
<pin name="LO" direction="out"/>
</symbol>
<symbol name="IRS2552DSPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VB" direction="pwr"/>
<pin name="ENA" direction="in"/>
<pin name="MAX" direction="in"/>
<pin name="MIN" direction="in"/>
<pin name="DIM" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="DT" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="CD" direction="in"/>
<pin name="SD" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="VS" direction="in"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS2573DSPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VBB" direction="in"/>
<pin name="VB1" direction="in"/>
<pin name="VB2" direction="in"/>
<pin name="VS1" direction="in"/>
<pin name="VS2" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="VSB" direction="in"/>
<pin name="TCLK" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="ZX" direction="in"/>
<pin name="TOFF" direction="in"/>
<pin name="ICOMP" direction="in"/>
<pin name="PCOMP" direction="in"/>
<pin name="IREF" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TIGN" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="OC" direction="in"/>
<pin name="VSENSE" direction="in"/>
<pin name="ISENCE" direction="in"/>
<pin name="OV" direction="in"/>
<pin name="BUCK" direction="out"/>
<pin name="IGN" direction="out"/>
<pin name="LO1" direction="out"/>
<pin name="LO2" direction="out"/>
<pin name="HO1" direction="out"/>
<pin name="HO2" direction="out"/>
</symbol>
<symbol name="IRS27951SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CT/SD" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
<symbol name="IRS27952SPBF">
<pin name="VCC" direction="pwr"/>
<pin name="VS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CT/SD" direction="in"/>
<pin name="VB" direction="in"/>
<pin name="COM" direction="pas"/>
<pin name="LO" direction="out"/>
<pin name="HO" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AUIR2085S" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="AUIR2085S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="4"/>
<connect gate="A" pin="OSC" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIR2085S"/>
<attribute name="OC_FARNELL" value="1866033"/>
<attribute name="OC_NEWARK" value="39T4047"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRF7343Q" prefix="U">
<description>AUTOMOTIVE MOSFET</description>
<gates>
<gate name="A" symbol="AUIRF7343Q"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D1" pad="8"/>
<connect gate="A" pin="D1_2" pad="7"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D2_2" pad="5"/>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="4"/>
<connect gate="A" pin="S1" pad="1"/>
<connect gate="A" pin="S2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRF7343Q"/>
<attribute name="OC_FARNELL" value="1865606"/>
<attribute name="OC_NEWARK" value="41T2748"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2004S" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS2004S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~SD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2004S"/>
<attribute name="OC_FARNELL" value="1866044"/>
<attribute name="OC_NEWARK" value="39T4028"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2016S" prefix="U">
<description>High Side Driver with Internal Vs Recharge</description>
<gates>
<gate name="A" symbol="AUIRS2016S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="RESET-" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2016S"/>
<attribute name="OC_FARNELL" value="1866045"/>
<attribute name="OC_NEWARK" value="39T4029"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2110S" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS2110S"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="12"/>
<connect gate="A" pin="HO" pad="8"/>
<connect gate="A" pin="LIN" pad="14"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="9"/>
<connect gate="A" pin="NC_4" pad="10"/>
<connect gate="A" pin="NC_5" pad="16"/>
<connect gate="A" pin="SD" pad="13"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2110S"/>
<attribute name="OC_FARNELL" value="1866046"/>
<attribute name="OC_NEWARK" value="39T4030"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2112S" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS2112S"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="12"/>
<connect gate="A" pin="HO" pad="8"/>
<connect gate="A" pin="LIN" pad="14"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="NC_5" pad="10"/>
<connect gate="A" pin="SD" pad="13"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2112S"/>
<attribute name="OC_FARNELL" value="1866048"/>
<attribute name="OC_NEWARK" value="39T4031"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2113S" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS2113S"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="12"/>
<connect gate="A" pin="HO" pad="8"/>
<connect gate="A" pin="LIN" pad="14"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="4"/>
<connect gate="A" pin="NC_4" pad="10"/>
<connect gate="A" pin="NC_5" pad="5"/>
<connect gate="A" pin="SD" pad="13"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2113S"/>
<attribute name="OC_FARNELL" value="1866049"/>
<attribute name="OC_NEWARK" value="39T4032"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2117S" prefix="U">
<description>SINGLE CHANNEL DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS2117S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2117S"/>
<attribute name="OC_FARNELL" value="1866050"/>
<attribute name="OC_NEWARK" value="39T4033"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2118S" prefix="U">
<description>SINGLE CHANNEL DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS2118S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~IN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2118S"/>
<attribute name="OC_FARNELL" value="1866051"/>
<attribute name="OC_NEWARK" value="39T4034"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS21271S" prefix="U">
<description>Over Current Protected Single Channel Driver</description>
<gates>
<gate name="A" symbol="AUIRS21271S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="~FAULT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS21271S"/>
<attribute name="OC_FARNELL" value="1866052"/>
<attribute name="OC_NEWARK" value="39T4035"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2127S" prefix="U">
<description>Over Current Protected Single Channel Driver</description>
<gates>
<gate name="A" symbol="AUIRS2127S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="~FAULT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2127S"/>
<attribute name="OC_FARNELL" value="1866053"/>
<attribute name="OC_NEWARK" value="41T2752"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS21281S" prefix="U">
<description>Over Current Protected Single Channel Driver</description>
<gates>
<gate name="A" symbol="AUIRS21281S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="~FAULT" pad="3"/>
<connect gate="A" pin="~IN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS21281S"/>
<attribute name="OC_FARNELL" value="1866054"/>
<attribute name="OC_NEWARK" value="39T4036"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2128S" prefix="U">
<description>Over Current Protected Single Channel Driver</description>
<gates>
<gate name="A" symbol="AUIRS2128S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="~FAULT" pad="3"/>
<connect gate="A" pin="~IN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2128S"/>
<attribute name="OC_FARNELL" value="1866055"/>
<attribute name="OC_NEWARK" value="41T2753"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS21811S" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS21811S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HIN" pad="1"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="2"/>
<connect gate="A" pin="LO" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS21811S"/>
<attribute name="OC_FARNELL" value="1866056"/>
<attribute name="OC_NEWARK" value="39T4038"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS21814S" prefix="U">
<description>HIGH- AND LOW-SIDE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS21814S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="COM" pad="5"/>
<connect gate="A" pin="HIN" pad="1"/>
<connect gate="A" pin="HO" pad="12"/>
<connect gate="A" pin="LIN" pad="2"/>
<connect gate="A" pin="LO" pad="6"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="14"/>
<connect gate="A" pin="NC_4" pad="8"/>
<connect gate="A" pin="NC_5" pad="9"/>
<connect gate="A" pin="VB" pad="13"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VS" pad="11"/>
<connect gate="A" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS21814S"/>
<attribute name="OC_FARNELL" value="1866057"/>
<attribute name="OC_NEWARK" value="39T4039"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2181S" prefix="U">
<description>HIGH- AND LOW-SIDE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS2181S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HIN" pad="1"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="2"/>
<connect gate="A" pin="LO" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2181S"/>
<attribute name="OC_FARNELL" value="1866058"/>
<attribute name="OC_NEWARK" value="39T4037"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS21844S" prefix="U">
<description>HIGH- AND LOW-SIDE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS21844S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="COM" pad="5"/>
<connect gate="A" pin="DT" pad="4"/>
<connect gate="A" pin="HO" pad="12"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="LO" pad="6"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="14"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="VB" pad="13"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VS" pad="11"/>
<connect gate="A" pin="VSS" pad="3"/>
<connect gate="A" pin="~SD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS21844S"/>
<attribute name="OC_FARNELL" value="1866061"/>
<attribute name="OC_NEWARK" value="39T4041"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2184S" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS2184S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="LO" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~SD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2184S"/>
<attribute name="OC_FARNELL" value="1866062"/>
<attribute name="OC_NEWARK" value="39T4040"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2191S" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS2191S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="COM" pad="9"/>
<connect gate="A" pin="HIN" pad="6"/>
<connect gate="A" pin="HO" pad="16"/>
<connect gate="A" pin="LIN" pad="7"/>
<connect gate="A" pin="LO" pad="11"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="2"/>
<connect gate="A" pin="NC_3" pad="3"/>
<connect gate="A" pin="NC_4" pad="4"/>
<connect gate="A" pin="NC_5" pad="5"/>
<connect gate="A" pin="NC_6" pad="10"/>
<connect gate="A" pin="NC_7" pad="13"/>
<connect gate="A" pin="VB" pad="1"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VS" pad="15"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2191S"/>
<attribute name="OC_FARNELL" value="1866063"/>
<attribute name="OC_NEWARK" value="39T4042"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2301S" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS2301S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="3"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2301S"/>
<attribute name="OC_FARNELL" value="1866064"/>
<attribute name="OC_NEWARK" value="39T4043"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS2302S" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS2302S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~SD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS2302S"/>
<attribute name="OC_FARNELL" value="1866065"/>
<attribute name="OC_NEWARK" value="39T4044"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS4426S" prefix="U">
<description>DUAL LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS4426S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="OUTA" pad="7"/>
<connect gate="A" pin="OUTB" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~INA" pad="2"/>
<connect gate="A" pin="~INB" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS4426S"/>
<attribute name="OC_FARNELL" value="1866066"/>
<attribute name="OC_NEWARK" value="39T4045"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUIRS4428S" prefix="U">
<description>DUAL LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="AUIRS4428S"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INB" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="OUTA" pad="7"/>
<connect gate="A" pin="OUTB" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~INA" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="AUIRS4428S"/>
<attribute name="OC_FARNELL" value="1866067"/>
<attribute name="OC_NEWARK" value="39T4046"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR1150IPBF" prefix="U">
<description>ìPFC ONE CYCLE CONTROL PFC IC</description>
<gates>
<gate name="A" symbol="IR1150IPBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="1"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="FREQ" pad="2"/>
<connect gate="A" pin="GATE" pad="8"/>
<connect gate="A" pin="ISNS" pad="3"/>
<connect gate="A" pin="OVP/EN" pad="4"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VFB" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR1150IPBF"/>
<attribute name="OC_FARNELL" value="1827117"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="DIP-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR1150ISTRPBF" prefix="U">
<description>uPFC ONE CYCLE CONTROL PFC IC</description>
<gates>
<gate name="A" symbol="IR1150ISTRPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="1"/>
<connect gate="A" pin="COMP" pad="5"/>
<connect gate="A" pin="FREQ" pad="2"/>
<connect gate="A" pin="GATE" pad="8"/>
<connect gate="A" pin="ISNS" pad="3"/>
<connect gate="A" pin="OVP/EN" pad="4"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VFB" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR1150ISTRPBF"/>
<attribute name="OC_FARNELL" value="1081506"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR11662SPBF" prefix="U">
<description>ADVANCED SMART RECTIFIER CONTROL IC</description>
<gates>
<gate name="A" symbol="IR11662SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="MOT" pad="3"/>
<connect gate="A" pin="OVT" pad="2"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VD" pad="5"/>
<connect gate="A" pin="VGATE" pad="8"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR11662SPBF"/>
<attribute name="OC_FARNELL" value="1866068"/>
<attribute name="OC_NEWARK" value="39T4530"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR11672ASPBF" prefix="U">
<description>ADVANCED SMART RECTIFIER CONTROL IC</description>
<gates>
<gate name="A" symbol="IR11672ASPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="EN" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="MOT" pad="3"/>
<connect gate="A" pin="OVT" pad="2"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VD" pad="5"/>
<connect gate="A" pin="VGATE" pad="8"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR11672ASPBF"/>
<attribute name="OC_FARNELL" value="1827123"/>
<attribute name="OC_NEWARK" value="84R4292"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR11682SPBF" prefix="U">
<description>DUAL SmartRectifier DRIVER IC</description>
<gates>
<gate name="A" symbol="IR11682SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GATE1" pad="1"/>
<connect gate="A" pin="GATE2" pad="8"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="VD1" pad="4"/>
<connect gate="A" pin="VD2" pad="5"/>
<connect gate="A" pin="VS1" pad="3"/>
<connect gate="A" pin="VS2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR11682SPBF"/>
<attribute name="OC_FARNELL" value="1866070"/>
<attribute name="OC_NEWARK" value="39T4531"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR1168SPBF" prefix="U">
<description>DUAL SMART RECTIFIER DRIVER IC</description>
<gates>
<gate name="A" symbol="IR1168SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GATE1" pad="1"/>
<connect gate="A" pin="GATE2" pad="8"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="VD1" pad="4"/>
<connect gate="A" pin="VD2" pad="5"/>
<connect gate="A" pin="VS1" pad="3"/>
<connect gate="A" pin="VS2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR1168SPBF"/>
<attribute name="OC_FARNELL" value="1827118"/>
<attribute name="OC_NEWARK" value="10R0385"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2010PBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2010PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-14">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="10"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="12"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="14"/>
<connect gate="A" pin="SD" pad="11"/>
<connect gate="A" pin="VB" pad="6"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="9"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2010PBF"/>
<attribute name="OC_FARNELL" value="1080609"/>
<attribute name="OC_NEWARK" value="19K8402"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2010SPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2010SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-16N">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="12"/>
<connect gate="A" pin="HO" pad="8"/>
<connect gate="A" pin="LIN" pad="14"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="10"/>
<connect gate="A" pin="NC_4" pad="16"/>
<connect gate="A" pin="NC_5" pad="5"/>
<connect gate="A" pin="SD" pad="13"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2010SPBF"/>
<attribute name="OC_FARNELL" value="1080610"/>
<attribute name="OC_NEWARK" value="19K8403"/>
<attribute name="PACKAGE" value="SOICW-16"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2011PBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2011PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HIN" pad="1"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="2"/>
<connect gate="A" pin="LO" pad="4"/>
<connect gate="A" pin="VB" pad="6"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2011PBF"/>
<attribute name="OC_FARNELL" value="1080612"/>
<attribute name="OC_NEWARK" value="41K2518"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2101PBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2101PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="3"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2101PBF"/>
<attribute name="OC_FARNELL" value="8638713"/>
<attribute name="OC_NEWARK" value="63J7837"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2102SPBF" prefix="U">
<description>DRIVER</description>
<gates>
<gate name="A" symbol="IR2102SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~HIN" pad="2"/>
<connect gate="A" pin="~LIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2102SPBF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="19K8406"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2103SPBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2103SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~LIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2103SPBF"/>
<attribute name="OC_FARNELL" value="8638730"/>
<attribute name="OC_NEWARK" value="63J7841"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2104PBF" prefix="U">
<description>HALF BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2104PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~SD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2104PBF"/>
<attribute name="OC_FARNELL" value="8638748"/>
<attribute name="OC_NEWARK" value="63J7843"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2104STRPBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2104STRPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~SD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2104STRPBF"/>
<attribute name="OC_FARNELL" value="1795566"/>
<attribute name="OC_NEWARK" value="40M8006"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2106SPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2106SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="3"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2106SPBF"/>
<attribute name="OC_FARNELL" value="8638799"/>
<attribute name="OC_NEWARK" value="-"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR21084SPBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR21084SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="COM" pad="6"/>
<connect gate="A" pin="DT" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="12"/>
<connect gate="A" pin="LO" pad="7"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="14"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="VB" pad="13"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="11"/>
<connect gate="A" pin="VSS" pad="5"/>
<connect gate="A" pin="~LIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR21084SPBF"/>
<attribute name="OC_FARNELL" value="9101810"/>
<attribute name="OC_NEWARK" value="19K8411"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2108PBF" prefix="U">
<description>HALF BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2108PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~LIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2108PBF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="19K8409"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2108SPBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2108SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~LIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2108SPBF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="63J7853"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2110-1PBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2110-1PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-14">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="10"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="12"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="SD" pad="11"/>
<connect gate="A" pin="VB" pad="6"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="9"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2110-1PBF"/>
<attribute name="OC_FARNELL" value="1374799"/>
<attribute name="OC_NEWARK" value="19K8414"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2110-2PBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2110-2PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-14">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="10"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="12"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="14"/>
<connect gate="A" pin="NC_3" pad="4"/>
<connect gate="A" pin="SD" pad="11"/>
<connect gate="A" pin="VB" pad="6"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="9"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2110-2PBF"/>
<attribute name="OC_FARNELL" value="1374834"/>
<attribute name="OC_NEWARK" value="31K2456"/>
<attribute name="PACKAGE" value="DIP-14"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2110PBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2110PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-14">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="10"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="12"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="14"/>
<connect gate="A" pin="SD" pad="11"/>
<connect gate="A" pin="VB" pad="6"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="9"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2110PBF"/>
<attribute name="OC_FARNELL" value="8638837"/>
<attribute name="OC_NEWARK" value="63J7859"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2110SPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2110SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="12"/>
<connect gate="A" pin="HO" pad="8"/>
<connect gate="A" pin="LIN" pad="14"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="NC_5" pad="16"/>
<connect gate="A" pin="SD" pad="13"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2110SPBF"/>
<attribute name="OC_FARNELL" value="8638845"/>
<attribute name="OC_NEWARK" value="63J7860"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2110STRPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2110STRPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-16N">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="12"/>
<connect gate="A" pin="HO" pad="8"/>
<connect gate="A" pin="LIN" pad="14"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="10"/>
<connect gate="A" pin="NC_4" pad="16"/>
<connect gate="A" pin="NC_5" pad="5"/>
<connect gate="A" pin="SD" pad="13"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2110STRPBF"/>
<attribute name="OC_FARNELL" value="8639680"/>
<attribute name="OC_NEWARK" value="40M8008"/>
<attribute name="PACKAGE" value="SOICW-16"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2111PBF" prefix="U">
<description>HALF BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2111PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="LO" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2111PBF"/>
<attribute name="OC_FARNELL" value="9101730"/>
<attribute name="OC_NEWARK" value="19K8415"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2111SPBF" prefix="U">
<description>SINGLE HIGH SIDE DRIVER IC</description>
<gates>
<gate name="A" symbol="IR2111SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2111SPBF"/>
<attribute name="OC_FARNELL" value="8638861"/>
<attribute name="OC_NEWARK" value="63J7862"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2111STRPBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2111STRPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="LO" pad="4"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2111STRPBF"/>
<attribute name="OC_FARNELL" value="8639698"/>
<attribute name="OC_NEWARK" value="40M8009"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2112PBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2112PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-14">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="10"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="12"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="14"/>
<connect gate="A" pin="SD" pad="11"/>
<connect gate="A" pin="VB" pad="6"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="9"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2112PBF"/>
<attribute name="OC_FARNELL" value="9101799"/>
<attribute name="OC_NEWARK" value="19K8417"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2112SPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2112SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="12"/>
<connect gate="A" pin="HO" pad="8"/>
<connect gate="A" pin="LIN" pad="14"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="NC_5" pad="16"/>
<connect gate="A" pin="SD" pad="13"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2112SPBF"/>
<attribute name="OC_FARNELL" value="8638870"/>
<attribute name="OC_NEWARK" value="63J7864"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2113PBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2113PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-14">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="10"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="12"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="14"/>
<connect gate="A" pin="SD" pad="11"/>
<connect gate="A" pin="VB" pad="6"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="9"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2113PBF"/>
<attribute name="OC_FARNELL" value="9101748"/>
<attribute name="OC_NEWARK" value="19K8418"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2113SPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2113SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="12"/>
<connect gate="A" pin="HO" pad="8"/>
<connect gate="A" pin="LIN" pad="14"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="NC_5" pad="16"/>
<connect gate="A" pin="SD" pad="13"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2113SPBF"/>
<attribute name="OC_FARNELL" value="8638888"/>
<attribute name="OC_NEWARK" value="63J7866"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2113STRPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2113STRPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-16N">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="12"/>
<connect gate="A" pin="HO" pad="8"/>
<connect gate="A" pin="LIN" pad="14"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="9"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="10"/>
<connect gate="A" pin="NC_4" pad="16"/>
<connect gate="A" pin="NC_5" pad="5"/>
<connect gate="A" pin="SD" pad="13"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2113STRPBF"/>
<attribute name="OC_FARNELL" value="8639710"/>
<attribute name="OC_NEWARK" value="40M8010"/>
<attribute name="PACKAGE" value="SOICW-16"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2117PBF" prefix="U">
<description>SINGLE CHANNEL DRIVER</description>
<gates>
<gate name="A" symbol="IR2117PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2117PBF"/>
<attribute name="OC_FARNELL" value="9101756"/>
<attribute name="OC_NEWARK" value="19K8419"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2117SPBF" prefix="U">
<description>SINGLE CHANNEL DRIVER</description>
<gates>
<gate name="A" symbol="IR2117SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2117SPBF"/>
<attribute name="OC_FARNELL" value="8638896"/>
<attribute name="OC_NEWARK" value="63J7868"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2118PBF" prefix="U">
<description>SINGLE CHANNEL DRIVER</description>
<gates>
<gate name="A" symbol="IR2118PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HO" pad="6"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="~IN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2118PBF"/>
<attribute name="OC_FARNELL" value="9101764"/>
<attribute name="OC_NEWARK" value="19K8420"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2118STRPBF" prefix="U">
<description>SINGLE CHANNEL DRIVER</description>
<gates>
<gate name="A" symbol="IR2118STRPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~IN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2118STRPBF"/>
<attribute name="OC_FARNELL" value="1795540"/>
<attribute name="OC_NEWARK" value="40M8012"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2121PBF" prefix="U">
<description>LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2121PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="ERR" pad="3"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VCC_2" pad="1"/>
<connect gate="A" pin="VS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2121PBF"/>
<attribute name="OC_FARNELL" value="9101705"/>
<attribute name="OC_NEWARK" value="63J7870"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2125PBF" prefix="U">
<description>SINGLE CHANNEL DRIVER</description>
<gates>
<gate name="A" symbol="IR2125PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="ERR" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2125PBF"/>
<attribute name="OC_FARNELL" value="9101721"/>
<attribute name="OC_NEWARK" value="19K8423"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR21271SPBF" prefix="U">
<description>Current Sensing Single Channel Driver</description>
<gates>
<gate name="A" symbol="IR21271SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="~FAULT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR21271SPBF"/>
<attribute name="OC_FARNELL" value="8638900"/>
<attribute name="OC_NEWARK" value="63J7873"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2127PBF" prefix="U">
<description>SINGLE CHANNEL DRIVER</description>
<gates>
<gate name="A" symbol="IR2127PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CS" pad="6"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="~FAULT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2127PBF"/>
<attribute name="OC_FARNELL" value="9101772"/>
<attribute name="OC_NEWARK" value="19K8425"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2130PBF" prefix="U">
<description>3-PHASE BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2130PBF"/>
</gates>
<devices>
<device name="" package="DIP254P1524X635-28">
<connects>
<connect gate="A" pin="CA-" pad="11"/>
<connect gate="A" pin="CA0" pad="10"/>
<connect gate="A" pin="HO1" pad="27"/>
<connect gate="A" pin="HO2" pad="23"/>
<connect gate="A" pin="HO3" pad="19"/>
<connect gate="A" pin="ITRIP" pad="9"/>
<connect gate="A" pin="LO1" pad="16"/>
<connect gate="A" pin="LO2" pad="15"/>
<connect gate="A" pin="LO3" pad="14"/>
<connect gate="A" pin="NC" pad="17"/>
<connect gate="A" pin="NC_2" pad="25"/>
<connect gate="A" pin="NC_3" pad="21"/>
<connect gate="A" pin="VB1" pad="28"/>
<connect gate="A" pin="VB2" pad="24"/>
<connect gate="A" pin="VB3" pad="20"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS0" pad="13"/>
<connect gate="A" pin="VS1" pad="26"/>
<connect gate="A" pin="VS2" pad="22"/>
<connect gate="A" pin="VS3" pad="18"/>
<connect gate="A" pin="VSS" pad="12"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~HIN1" pad="2"/>
<connect gate="A" pin="~HIN2" pad="3"/>
<connect gate="A" pin="~HIN3" pad="4"/>
<connect gate="A" pin="~LIN1" pad="5"/>
<connect gate="A" pin="~LIN2" pad="6"/>
<connect gate="A" pin="~LIN3" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2130PBF"/>
<attribute name="OC_FARNELL" value="1822292"/>
<attribute name="OC_NEWARK" value="88K5094"/>
<attribute name="PACKAGE" value="PCDIP-28"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2130SPBF" prefix="U">
<description>3-PHASE BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2130SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127PX1032X265-28N">
<connects>
<connect gate="A" pin="CA-" pad="11"/>
<connect gate="A" pin="CAO" pad="10"/>
<connect gate="A" pin="HO1" pad="27"/>
<connect gate="A" pin="HO2" pad="23"/>
<connect gate="A" pin="HO3" pad="19"/>
<connect gate="A" pin="ITRIP" pad="9"/>
<connect gate="A" pin="LO1" pad="16"/>
<connect gate="A" pin="LO2" pad="15"/>
<connect gate="A" pin="LO3" pad="14"/>
<connect gate="A" pin="VB1" pad="28"/>
<connect gate="A" pin="VB2" pad="24"/>
<connect gate="A" pin="VB3" pad="20"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS1" pad="26"/>
<connect gate="A" pin="VS2" pad="22"/>
<connect gate="A" pin="VS3" pad="18"/>
<connect gate="A" pin="VSO" pad="13"/>
<connect gate="A" pin="VSS" pad="12"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~HIN1" pad="2"/>
<connect gate="A" pin="~HIN2" pad="3"/>
<connect gate="A" pin="~HIN3" pad="4"/>
<connect gate="A" pin="~LIN1" pad="5"/>
<connect gate="A" pin="~LIN2" pad="6"/>
<connect gate="A" pin="~LIN3" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2130SPBF"/>
<attribute name="OC_FARNELL" value="9101845"/>
<attribute name="OC_NEWARK" value="58K5837"/>
<attribute name="PACKAGE" value="SOIC28"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2131SPBF" prefix="U">
<description>3 HIGH SIDE AND 3 LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2131SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127PX1032X265-28N">
<connects>
<connect gate="A" pin="COM" pad="13"/>
<connect gate="A" pin="HO1" pad="27"/>
<connect gate="A" pin="HO2" pad="23"/>
<connect gate="A" pin="HO3" pad="19"/>
<connect gate="A" pin="ITRIP" pad="9"/>
<connect gate="A" pin="LO1" pad="16"/>
<connect gate="A" pin="LO2" pad="15"/>
<connect gate="A" pin="LO3" pad="14"/>
<connect gate="A" pin="SD" pad="11"/>
<connect gate="A" pin="VB1" pad="28"/>
<connect gate="A" pin="VB2" pad="24"/>
<connect gate="A" pin="VB3" pad="20"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS1" pad="26"/>
<connect gate="A" pin="VS2" pad="22"/>
<connect gate="A" pin="VS3" pad="18"/>
<connect gate="A" pin="VSS" pad="12"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~FLT-CLR" pad="10"/>
<connect gate="A" pin="~HIN1" pad="2"/>
<connect gate="A" pin="~HIN2" pad="3"/>
<connect gate="A" pin="~HIN3" pad="4"/>
<connect gate="A" pin="~LIN1" pad="5"/>
<connect gate="A" pin="~LIN2" pad="6"/>
<connect gate="A" pin="~LIN3" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2131SPBF"/>
<attribute name="OC_FARNELL" value="1023211"/>
<attribute name="OC_NEWARK" value="19K8427"/>
<attribute name="PACKAGE" value="SOIC28"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2132SPBF" prefix="U">
<description>3-PHASE BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2132SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127PX1032X265-28N">
<connects>
<connect gate="A" pin="CA-" pad="11"/>
<connect gate="A" pin="CAO" pad="10"/>
<connect gate="A" pin="HO1" pad="27"/>
<connect gate="A" pin="HO2" pad="23"/>
<connect gate="A" pin="HO3" pad="19"/>
<connect gate="A" pin="ITRIP" pad="9"/>
<connect gate="A" pin="LO1" pad="16"/>
<connect gate="A" pin="LO2" pad="15"/>
<connect gate="A" pin="LO3" pad="14"/>
<connect gate="A" pin="VB1" pad="28"/>
<connect gate="A" pin="VB2" pad="24"/>
<connect gate="A" pin="VB3" pad="20"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS1" pad="26"/>
<connect gate="A" pin="VS2" pad="22"/>
<connect gate="A" pin="VS3" pad="18"/>
<connect gate="A" pin="VSO" pad="13"/>
<connect gate="A" pin="VSS" pad="12"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~HIN1" pad="2"/>
<connect gate="A" pin="~HIN2" pad="3"/>
<connect gate="A" pin="~HIN3" pad="4"/>
<connect gate="A" pin="~LIN1" pad="5"/>
<connect gate="A" pin="~LIN2" pad="6"/>
<connect gate="A" pin="~LIN3" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2132SPBF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="63J7876"/>
<attribute name="PACKAGE" value="SOIC28"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR21362PBF" prefix="U">
<description>3-PHASE BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR21362PBF"/>
</gates>
<devices>
<device name="" package="DIP254P1524X635-28">
<connects>
<connect gate="A" pin="COM" pad="13"/>
<connect gate="A" pin="EN" pad="10"/>
<connect gate="A" pin="HIN1" pad="2"/>
<connect gate="A" pin="HIN2" pad="3"/>
<connect gate="A" pin="HIN3" pad="4"/>
<connect gate="A" pin="HO1" pad="27"/>
<connect gate="A" pin="HO2" pad="23"/>
<connect gate="A" pin="HO3" pad="19"/>
<connect gate="A" pin="ITRIP" pad="9"/>
<connect gate="A" pin="LO1" pad="16"/>
<connect gate="A" pin="LO2" pad="15"/>
<connect gate="A" pin="LO3" pad="14"/>
<connect gate="A" pin="NC" pad="17"/>
<connect gate="A" pin="NC_2" pad="25"/>
<connect gate="A" pin="NC_3" pad="21"/>
<connect gate="A" pin="RCIN" pad="11"/>
<connect gate="A" pin="VB1" pad="28"/>
<connect gate="A" pin="VB2" pad="24"/>
<connect gate="A" pin="VB3" pad="20"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS1" pad="26"/>
<connect gate="A" pin="VS2" pad="22"/>
<connect gate="A" pin="VS3" pad="18"/>
<connect gate="A" pin="VSS" pad="12"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~LIN1" pad="5"/>
<connect gate="A" pin="~LIN2" pad="6"/>
<connect gate="A" pin="~LIN3" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR21362PBF"/>
<attribute name="OC_FARNELL" value="1023217"/>
<attribute name="OC_NEWARK" value="33K5196"/>
<attribute name="PACKAGE" value="PDIP-28"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2136SPBF" prefix="U">
<description>3-PHASE BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2136SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127PX1032X265-28N">
<connects>
<connect gate="A" pin="COM" pad="13"/>
<connect gate="A" pin="EN" pad="10"/>
<connect gate="A" pin="HIN1" pad="2"/>
<connect gate="A" pin="HIN2" pad="3"/>
<connect gate="A" pin="HIN3" pad="4"/>
<connect gate="A" pin="HO1" pad="27"/>
<connect gate="A" pin="HO2" pad="23"/>
<connect gate="A" pin="HO3" pad="19"/>
<connect gate="A" pin="ITRIP" pad="9"/>
<connect gate="A" pin="LO1" pad="16"/>
<connect gate="A" pin="LO2" pad="15"/>
<connect gate="A" pin="LO3" pad="14"/>
<connect gate="A" pin="RCIN" pad="11"/>
<connect gate="A" pin="VB1" pad="28"/>
<connect gate="A" pin="VB2" pad="24"/>
<connect gate="A" pin="VB3" pad="20"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS1" pad="26"/>
<connect gate="A" pin="VS2" pad="22"/>
<connect gate="A" pin="VS3" pad="18"/>
<connect gate="A" pin="VSS" pad="12"/>
<connect gate="A" pin="~FAULT" pad="8"/>
<connect gate="A" pin="~LIN1" pad="5"/>
<connect gate="A" pin="~LIN2" pad="6"/>
<connect gate="A" pin="~LIN3" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2136SPBF"/>
<attribute name="OC_FARNELL" value="8638950"/>
<attribute name="OC_NEWARK" value="63J7880"/>
<attribute name="PACKAGE" value="SOIC28"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR21531DPBF" prefix="U">
<description>HALF BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR21531DPBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR21531DPBF"/>
<attribute name="OC_FARNELL" value="1375200"/>
<attribute name="OC_NEWARK" value="73K8366"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2153DPBF" prefix="U">
<description>HALF BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2153DPBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2153DPBF"/>
<attribute name="OC_FARNELL" value="9101861"/>
<attribute name="OC_NEWARK" value="19K8435"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2153PBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2153PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2153PBF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="63J7894"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR21834STRPBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR21834STRPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="COM" pad="5"/>
<connect gate="A" pin="DT" pad="4"/>
<connect gate="A" pin="HIN" pad="1"/>
<connect gate="A" pin="HO" pad="12"/>
<connect gate="A" pin="LO" pad="6"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="9"/>
<connect gate="A" pin="NC_4" pad="10"/>
<connect gate="A" pin="VB" pad="13"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VS" pad="11"/>
<connect gate="A" pin="VSS" pad="3"/>
<connect gate="A" pin="~LIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR21834STRPBF"/>
<attribute name="OC_FARNELL" value="1375038"/>
<attribute name="OC_NEWARK" value="40M8014"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2183PBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2183PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HIN" pad="1"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~LIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2183PBF"/>
<attribute name="OC_FARNELL" value="1023246"/>
<attribute name="OC_NEWARK" value="19K8447"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR21844SPBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR21844SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="COM" pad="5"/>
<connect gate="A" pin="DT" pad="4"/>
<connect gate="A" pin="HO" pad="12"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="LO" pad="6"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="14"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="VB" pad="13"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VS" pad="11"/>
<connect gate="A" pin="VSS" pad="3"/>
<connect gate="A" pin="~SD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR21844SPBF"/>
<attribute name="OC_FARNELL" value="8639043"/>
<attribute name="OC_NEWARK" value="63J7908"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2184PBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IR2184PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="LO" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~SD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2184PBF"/>
<attribute name="OC_FARNELL" value="1023249"/>
<attribute name="OC_NEWARK" value="19K8450"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2213PBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2213PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-14">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="10"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="12"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="4"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="14"/>
<connect gate="A" pin="SD" pad="11"/>
<connect gate="A" pin="VB" pad="6"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="9"/>
<connect gate="A" pin="VS" pad="5"/>
<connect gate="A" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2213PBF"/>
<attribute name="OC_FARNELL" value="1023250"/>
<attribute name="OC_NEWARK" value="19K8452"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR2213SPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR2213SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-16N">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="HIN" pad="12"/>
<connect gate="A" pin="HO" pad="8"/>
<connect gate="A" pin="LIN" pad="14"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="5"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="NC_5" pad="16"/>
<connect gate="A" pin="SD" pad="13"/>
<connect gate="A" pin="VB" pad="7"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="A" pin="VDD" pad="11"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR2213SPBF"/>
<attribute name="OC_FARNELL" value="1023252"/>
<attribute name="OC_NEWARK" value="19K8453"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR4426PBF" prefix="U">
<description>DUAL LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR4426PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="OUTA" pad="7"/>
<connect gate="A" pin="OUTB" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~INA" pad="2"/>
<connect gate="A" pin="~INB" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR4426PBF"/>
<attribute name="OC_FARNELL" value="1023265"/>
<attribute name="OC_NEWARK" value="19K8460"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR4427PBF" prefix="U">
<description>DUAL LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR4427PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INA" pad="2"/>
<connect gate="A" pin="INB" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="OUTA" pad="7"/>
<connect gate="A" pin="OUTB" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR4427PBF"/>
<attribute name="OC_FARNELL" value="1023267"/>
<attribute name="OC_NEWARK" value="19K8462"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR4427SPBF" prefix="U">
<description>DUAL LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR4427SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INA" pad="2"/>
<connect gate="A" pin="INB" pad="4"/>
<connect gate="A" pin="NC" pad="8"/>
<connect gate="A" pin="NC_2" pad="1"/>
<connect gate="A" pin="OUTA" pad="7"/>
<connect gate="A" pin="OUTB" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR4427SPBF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="19K8463"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR4428PBF" prefix="U">
<description>DUAL LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IR4428PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="INB" pad="4"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="OUTA" pad="7"/>
<connect gate="A" pin="OUTB" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~INA" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IR4428PBF"/>
<attribute name="OC_FARNELL" value="1023268"/>
<attribute name="OC_NEWARK" value="19K8464"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRF7815PBF" prefix="U">
<description>HEXFET Power MOSFET</description>
<gates>
<gate name="A" symbol="IRF7815PBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="D_2" pad="7"/>
<connect gate="A" pin="D_3" pad="8"/>
<connect gate="A" pin="D_4" pad="5"/>
<connect gate="A" pin="G" pad="4"/>
<connect gate="A" pin="S" pad="2"/>
<connect gate="A" pin="S_2" pad="1"/>
<connect gate="A" pin="S_3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRF7815PBF"/>
<attribute name="OC_FARNELL" value="1865585"/>
<attribute name="OC_NEWARK" value="57R4071"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRF9332PBF" prefix="U">
<description>HEXFET Power MOSFET</description>
<gates>
<gate name="A" symbol="IRF9332PBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="D_2" pad="7"/>
<connect gate="A" pin="D_3" pad="8"/>
<connect gate="A" pin="D_4" pad="5"/>
<connect gate="A" pin="G" pad="4"/>
<connect gate="A" pin="S" pad="2"/>
<connect gate="A" pin="S_2" pad="1"/>
<connect gate="A" pin="S_3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRF9332PBF"/>
<attribute name="OC_FARNELL" value="1857354"/>
<attribute name="OC_NEWARK" value="12T9892"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRF9358PBF" prefix="U">
<description>HEXFET Power MOSFET</description>
<gates>
<gate name="A" symbol="IRF9358PBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D1" pad="6"/>
<connect gate="A" pin="D1_2" pad="5"/>
<connect gate="A" pin="D2" pad="8"/>
<connect gate="A" pin="D2_2" pad="7"/>
<connect gate="A" pin="G1" pad="4"/>
<connect gate="A" pin="G2" pad="2"/>
<connect gate="A" pin="S1" pad="3"/>
<connect gate="A" pin="S2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRF9358PBF"/>
<attribute name="OC_FARNELL" value="1864523"/>
<attribute name="OC_NEWARK" value="25T5523"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRF9362PBF" prefix="U">
<description>HEXFET Power MOSFET</description>
<gates>
<gate name="A" symbol="IRF9362PBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D1" pad="8"/>
<connect gate="A" pin="D1_2" pad="7"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D2_2" pad="5"/>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="4"/>
<connect gate="A" pin="S1" pad="1"/>
<connect gate="A" pin="S2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRF9362PBF"/>
<attribute name="OC_FARNELL" value="1857301"/>
<attribute name="OC_NEWARK" value="79R7563"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRFML8244TRPBF" prefix="U">
<description>Power MOSFET</description>
<gates>
<gate name="A" symbol="IRFML8244TRPBF"/>
</gates>
<devices>
<device name="" package="SOT95P240X112-3N">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRFML8244TRPBF"/>
<attribute name="OC_FARNELL" value="1857298"/>
<attribute name="OC_NEWARK" value="25T5496"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRL6342PBF" prefix="U">
<description>HEXFETPower MOSFET</description>
<gates>
<gate name="A" symbol="IRL6342PBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="D" pad="8"/>
<connect gate="A" pin="D_2" pad="5"/>
<connect gate="A" pin="D_3" pad="6"/>
<connect gate="A" pin="D_4" pad="7"/>
<connect gate="A" pin="G" pad="4"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="A" pin="S_2" pad="1"/>
<connect gate="A" pin="S_3" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRL6342PBF"/>
<attribute name="OC_FARNELL" value="1890091"/>
<attribute name="OC_NEWARK" value="25T5535"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONALRECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRLML2244TRPBF" prefix="U">
<description>HEXFET Power MOSFET</description>
<gates>
<gate name="A" symbol="IRLML2244TRPBF"/>
</gates>
<devices>
<device name="" package="SOT95P237X112-3N">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRLML2244TRPBF"/>
<attribute name="OC_FARNELL" value="1888165"/>
<attribute name="OC_NEWARK" value="40T7448"/>
<attribute name="PACKAGE" value="SOT-3"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRLML2246TRPBF" prefix="U">
<description>HEXFET Power MOSFET</description>
<gates>
<gate name="A" symbol="IRLML2246TRPBF"/>
</gates>
<devices>
<device name="" package="SOT95P237X112-3N">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRLML2246TRPBF"/>
<attribute name="OC_FARNELL" value="1888166"/>
<attribute name="OC_NEWARK" value="40T7450"/>
<attribute name="PACKAGE" value="SOT-3"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRLML6244TRPBF" prefix="U">
<description>HEXFET Power MOSFET</description>
<gates>
<gate name="A" symbol="IRLML6244TRPBF"/>
</gates>
<devices>
<device name="" package="SOT95P237X112-3N">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRLML6244TRPBF"/>
<attribute name="OC_FARNELL" value="1864517"/>
<attribute name="OC_NEWARK" value="84R9705"/>
<attribute name="PACKAGE" value="SOT-3"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRLML6246TRPBF" prefix="U">
<description>Power MOSFET</description>
<gates>
<gate name="A" symbol="IRLML6246TRPBF"/>
</gates>
<devices>
<device name="" package="SOT95P240X112-3N">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRLML6246TRPBF"/>
<attribute name="OC_FARNELL" value="1857343"/>
<attribute name="OC_NEWARK" value="84R9707"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRLML6344TRPBF" prefix="U">
<description>Power MOSFET</description>
<gates>
<gate name="A" symbol="IRLML6344TRPBF"/>
</gates>
<devices>
<device name="" package="SOT95P240X112-3N">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRLML6344TRPBF"/>
<attribute name="OC_FARNELL" value="1857299"/>
<attribute name="OC_NEWARK" value="25T5501"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRLML6346TRPBF" prefix="U">
<description>Power MOSFET</description>
<gates>
<gate name="A" symbol="IRLML6346TRPBF"/>
</gates>
<devices>
<device name="" package="SOT95P240X112-3N">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRLML6346TRPBF"/>
<attribute name="OC_FARNELL" value="1857300"/>
<attribute name="OC_NEWARK" value="25T5502"/>
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2001SPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IRS2001SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="3"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2001SPBF"/>
<attribute name="OC_FARNELL" value="1603666"/>
<attribute name="OC_NEWARK" value="21M6577"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2003PBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IRS2003PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~LIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2003PBF"/>
<attribute name="OC_FARNELL" value="1603667"/>
<attribute name="OC_NEWARK" value="21M6590"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2003SPBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IRS2003SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~LIN" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2003SPBF"/>
<attribute name="OC_FARNELL" value="1603669"/>
<attribute name="OC_NEWARK" value="21M6591"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2011SPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IRS2011SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="7"/>
<connect gate="A" pin="HIN" pad="5"/>
<connect gate="A" pin="HO" pad="3"/>
<connect gate="A" pin="LIN" pad="6"/>
<connect gate="A" pin="LO" pad="8"/>
<connect gate="A" pin="VB" pad="2"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2011SPBF"/>
<attribute name="OC_FARNELL" value="1080636"/>
<attribute name="OC_NEWARK" value="58K5829"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS20124SPBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IRS20124SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="COM" pad="6"/>
<connect gate="A" pin="DT/SD" pad="3"/>
<connect gate="A" pin="HO" pad="11"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="LO" pad="7"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="9"/>
<connect gate="A" pin="NC_3" pad="13"/>
<connect gate="A" pin="OCSET1" pad="2"/>
<connect gate="A" pin="OCSET2" pad="4"/>
<connect gate="A" pin="VB" pad="12"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="VS" pad="10"/>
<connect gate="A" pin="~OC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS20124SPBF"/>
<attribute name="OC_FARNELL" value="1080637"/>
<attribute name="OC_NEWARK" value="58K5831"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2092PBF" prefix="U">
<description>PROTECTED DIGITAL AUDIO AMPLIFIER</description>
<gates>
<gate name="A" symbol="IRS2092PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-16">
<connects>
<connect gate="A" pin="COMP" pad="10"/>
<connect gate="A" pin="COMP_2" pad="4"/>
<connect gate="A" pin="CSD" pad="5"/>
<connect gate="A" pin="CSH" pad="16"/>
<connect gate="A" pin="DT" pad="9"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="HO" pad="14"/>
<connect gate="A" pin="IN-" pad="3"/>
<connect gate="A" pin="LO" pad="11"/>
<connect gate="A" pin="OCSET" pad="8"/>
<connect gate="A" pin="VAA" pad="1"/>
<connect gate="A" pin="VB" pad="15"/>
<connect gate="A" pin="VCC" pad="12"/>
<connect gate="A" pin="VREF" pad="7"/>
<connect gate="A" pin="VS" pad="13"/>
<connect gate="A" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2092PBF"/>
<attribute name="OC_FARNELL" value="1688533"/>
<attribute name="OC_NEWARK" value="02P2146"/>
<attribute name="PACKAGE" value="DIP-16"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS20957SPBF" prefix="U">
<description>Protected Digital Audio Driver</description>
<gates>
<gate name="A" symbol="IRS20957SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="COM" pad="9"/>
<connect gate="A" pin="CSD" pad="2"/>
<connect gate="A" pin="CSH" pad="16"/>
<connect gate="A" pin="DT" pad="8"/>
<connect gate="A" pin="HO" pad="14"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="LO" pad="10"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="12"/>
<connect gate="A" pin="OCSET" pad="7"/>
<connect gate="A" pin="VB" pad="15"/>
<connect gate="A" pin="VCC" pad="11"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VREF" pad="6"/>
<connect gate="A" pin="VS" pad="13"/>
<connect gate="A" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS20957SPBF"/>
<attribute name="OC_FARNELL" value="1695906"/>
<attribute name="OC_NEWARK" value="51P1630"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2153DPBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IRS2153DPBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2153DPBF"/>
<attribute name="OC_FARNELL" value="1271804"/>
<attribute name="OC_NEWARK" value="88K5081"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS21844PBF" prefix="U">
<description>HALF-BRIDGE DRIVER</description>
<gates>
<gate name="A" symbol="IRS21844PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-14">
<connects>
<connect gate="A" pin="COM" pad="5"/>
<connect gate="A" pin="DT" pad="4"/>
<connect gate="A" pin="HO" pad="12"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="LO" pad="6"/>
<connect gate="A" pin="NC" pad="14"/>
<connect gate="A" pin="NC_2" pad="10"/>
<connect gate="A" pin="NC_3" pad="8"/>
<connect gate="A" pin="NC_4" pad="9"/>
<connect gate="A" pin="VB" pad="13"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VS" pad="11"/>
<connect gate="A" pin="VSS" pad="3"/>
<connect gate="A" pin="~SD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS21844PBF"/>
<attribute name="OC_FARNELL" value="1271815"/>
<attribute name="OC_NEWARK" value="11M1885"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS21851SPBF" prefix="U">
<description>SINGLE HIGH SIDE DRIVER IC</description>
<gates>
<gate name="A" symbol="IRS21851SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="NC" pad="5"/>
<connect gate="A" pin="NC_2" pad="3"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS21851SPBF"/>
<attribute name="OC_FARNELL" value="1498206"/>
<attribute name="OC_NEWARK" value="21M6606"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS21864PBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IRS21864PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-14">
<connects>
<connect gate="A" pin="COM" pad="5"/>
<connect gate="A" pin="HIN" pad="1"/>
<connect gate="A" pin="HO" pad="12"/>
<connect gate="A" pin="LIN" pad="2"/>
<connect gate="A" pin="LO" pad="6"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="8"/>
<connect gate="A" pin="NC_3" pad="9"/>
<connect gate="A" pin="NC_4" pad="14"/>
<connect gate="A" pin="NC_5" pad="4"/>
<connect gate="A" pin="VB" pad="13"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VS" pad="11"/>
<connect gate="A" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS21864PBF"/>
<attribute name="OC_FARNELL" value="1688538"/>
<attribute name="OC_NEWARK" value="21M6613"/>
<attribute name="PACKAGE" value="PDIP-14"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS21864SPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IRS21864SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-14N">
<connects>
<connect gate="A" pin="COM" pad="5"/>
<connect gate="A" pin="HIN" pad="1"/>
<connect gate="A" pin="HO" pad="12"/>
<connect gate="A" pin="LO" pad="6"/>
<connect gate="A" pin="NC" pad="10"/>
<connect gate="A" pin="NC_2" pad="4"/>
<connect gate="A" pin="NC_3" pad="14"/>
<connect gate="A" pin="NC_4" pad="8"/>
<connect gate="A" pin="NC_5" pad="9"/>
<connect gate="A" pin="VB" pad="13"/>
<connect gate="A" pin="VCC" pad="7"/>
<connect gate="A" pin="VS" pad="11"/>
<connect gate="A" pin="VSS" pad="3"/>
<connect gate="A" pin="~LIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS21864SPBF"/>
<attribute name="OC_FARNELL" value="1688539"/>
<attribute name="OC_NEWARK" value="21M6614"/>
<attribute name="PACKAGE" value="SOIC-14"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2186PBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IRS2186PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HIN" pad="1"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
<connect gate="A" pin="~LIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2186PBF"/>
<attribute name="OC_FARNELL" value="1688540"/>
<attribute name="OC_NEWARK" value="21M6609"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2186STRPBF" prefix="U">
<description>HIGH AND LOW SIDE DRIVER</description>
<gates>
<gate name="A" symbol="IRS2186STRPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="3"/>
<connect gate="A" pin="HIN" pad="1"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LIN" pad="2"/>
<connect gate="A" pin="LO" pad="4"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2186STRPBF"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="21M6611"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS21952SPBF" prefix="U">
<description>HIGH SIDE &amp; DUAL LOW SIDE DRIVER IC</description>
<gates>
<gate name="A" symbol="IRS21952SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="COM" pad="9"/>
<connect gate="A" pin="HIN" pad="2"/>
<connect gate="A" pin="HO" pad="15"/>
<connect gate="A" pin="LIN1" pad="3"/>
<connect gate="A" pin="LIN2" pad="4"/>
<connect gate="A" pin="LO1" pad="8"/>
<connect gate="A" pin="LO2" pad="10"/>
<connect gate="A" pin="NC" pad="6"/>
<connect gate="A" pin="NC_2" pad="12"/>
<connect gate="A" pin="NC_3" pad="13"/>
<connect gate="A" pin="NC_4" pad="7"/>
<connect gate="A" pin="VB" pad="16"/>
<connect gate="A" pin="VCC" pad="11"/>
<connect gate="A" pin="VDD" pad="1"/>
<connect gate="A" pin="VS" pad="14"/>
<connect gate="A" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS21952SPBF"/>
<attribute name="OC_FARNELL" value="1925166"/>
<attribute name="OC_NEWARK" value="47P5816"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2541PBF" prefix="U">
<description>LED BUCK REGULATOR CONTROL IC</description>
<gates>
<gate name="A" symbol="IRS2541PBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="ENN" pad="4"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="IFB" pad="3"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2541PBF"/>
<attribute name="OC_FARNELL" value="1328477"/>
<attribute name="OC_NEWARK" value="18M5024"/>
<attribute name="PACKAGE" value="PDIP"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2552DPBF" prefix="U">
<description>CCFL/EEFL BALLAST CONTROLLER</description>
<gates>
<gate name="A" symbol="IRS2552DPBF"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-16">
<connects>
<connect gate="A" pin="CD" pad="10"/>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="CR" pad="9"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="DIM" pad="7"/>
<connect gate="A" pin="DT" pad="4"/>
<connect gate="A" pin="ENA" pad="8"/>
<connect gate="A" pin="HO" pad="15"/>
<connect gate="A" pin="LO" pad="13"/>
<connect gate="A" pin="MAX" pad="6"/>
<connect gate="A" pin="MIN" pad="5"/>
<connect gate="A" pin="SD" pad="11"/>
<connect gate="A" pin="VB" pad="16"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2552DPBF"/>
<attribute name="OC_FARNELL" value="1866039"/>
<attribute name="OC_NEWARK" value="39T4527"/>
<attribute name="PACKAGE" value="DIP-16"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2552DSPBF" prefix="U">
<description>CCFL/EEFL BALLAST CONTROLLER IC</description>
<gates>
<gate name="A" symbol="IRS2552DSPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-16N">
<connects>
<connect gate="A" pin="CD" pad="10"/>
<connect gate="A" pin="COM" pad="2"/>
<connect gate="A" pin="CR" pad="9"/>
<connect gate="A" pin="CS" pad="12"/>
<connect gate="A" pin="CT" pad="3"/>
<connect gate="A" pin="DIM" pad="7"/>
<connect gate="A" pin="DT" pad="4"/>
<connect gate="A" pin="ENA" pad="8"/>
<connect gate="A" pin="HO" pad="15"/>
<connect gate="A" pin="LO" pad="13"/>
<connect gate="A" pin="MAX" pad="6"/>
<connect gate="A" pin="MIN" pad="5"/>
<connect gate="A" pin="SD" pad="11"/>
<connect gate="A" pin="VB" pad="16"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2552DSPBF"/>
<attribute name="OC_FARNELL" value="1866040"/>
<attribute name="OC_NEWARK" value="39T4528"/>
<attribute name="PACKAGE" value="SOIC-16"/>
<attribute name="SUPPLIER" value="International Rectifier"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS2573DSPBF" prefix="U">
<description>HID BALLAST CONTROL IC</description>
<gates>
<gate name="A" symbol="IRS2573DSPBF"/>
</gates>
<devices>
<device name="" package="SOIC127PX1032X265-28N">
<connects>
<connect gate="A" pin="BUCK" pad="2"/>
<connect gate="A" pin="COM" pad="6"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="CT" pad="12"/>
<connect gate="A" pin="HO1" pad="27"/>
<connect gate="A" pin="HO2" pad="22"/>
<connect gate="A" pin="ICOMP" pad="9"/>
<connect gate="A" pin="IGN" pad="20"/>
<connect gate="A" pin="IREF" pad="11"/>
<connect gate="A" pin="ISENCE" pad="17"/>
<connect gate="A" pin="LO1" pad="25"/>
<connect gate="A" pin="LO2" pad="24"/>
<connect gate="A" pin="OC" pad="18"/>
<connect gate="A" pin="OV" pad="19"/>
<connect gate="A" pin="PCOMP" pad="10"/>
<connect gate="A" pin="RST" pad="15"/>
<connect gate="A" pin="TCLK" pad="14"/>
<connect gate="A" pin="TIGN" pad="13"/>
<connect gate="A" pin="TOFF" pad="8"/>
<connect gate="A" pin="VB1" pad="28"/>
<connect gate="A" pin="VB2" pad="23"/>
<connect gate="A" pin="VBB" pad="4"/>
<connect gate="A" pin="VCC" pad="5"/>
<connect gate="A" pin="VS1" pad="26"/>
<connect gate="A" pin="VS2" pad="21"/>
<connect gate="A" pin="VSB" pad="3"/>
<connect gate="A" pin="VSENSE" pad="16"/>
<connect gate="A" pin="ZX" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS2573DSPBF"/>
<attribute name="OC_FARNELL" value="1866041"/>
<attribute name="OC_NEWARK" value="41T2874"/>
<attribute name="PACKAGE" value="SOIC-28"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS27951SPBF" prefix="U">
<description>RESONANT HALF-BRIDGE CONVERTER CONTROL IC</description>
<gates>
<gate name="A" symbol="IRS27951SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CT/SD" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS27951SPBF"/>
<attribute name="OC_FARNELL" value="1866042"/>
<attribute name="OC_NEWARK" value="39T4529"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRS27952SPBF" prefix="U">
<description>RESONANT HALF-BRIDGE CONVERTER CONTROL IC</description>
<gates>
<gate name="A" symbol="IRS27952SPBF"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="COM" pad="4"/>
<connect gate="A" pin="CT/SD" pad="3"/>
<connect gate="A" pin="HO" pad="7"/>
<connect gate="A" pin="LO" pad="5"/>
<connect gate="A" pin="RT" pad="2"/>
<connect gate="A" pin="VB" pad="8"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="IRS27952SPBF"/>
<attribute name="OC_FARNELL" value="1866043"/>
<attribute name="OC_NEWARK" value="41T2875"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="INTERNATIONAL RECTIFIER"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
