| back |  | Last regenerated: 2022-04-20 17:31:36 kio

# zasm - Z80 Assembler – Version 4.4

# Targets

[<prev] [next>]

| ### #target TZX #### 0x31: Message block
    #tzx MESSAGE, [DURATION=]duration, [TEXT=]text
Display a message during loading. DURATION: time to display this message in seconds. TEXT: Ascii text. At most 8 lines à 30 characters. Text lines must be enclosed in quotes and lines separated by comma. #insert: Examples: #assert: Example: incbin: Examples: #assert: Example:Example
    #tzx message, 5, "Hello world,","this is a test message.","cheese."

[<prev] [top] [next>]