| back |  | Last regenerated: 2022-04-20 17:31:36 kio

# zasm - Z80 Assembler – Version 4.4

# Pseudo instructions

[<prev] [next>]

| ### defw, dw, .dw, .word
    defw  <value> [,<value>...]
    Pseudo instructions: defw, dw, .dw, .word
    8080 pseudo instructions: DWdw    <value> [,<value>...]
    .Pseudo instructions: defw, dw, .dw, .word
    8080 pseudo instructions: DWdw   <value> [,<value>...]
    .word <value> [,<value>...]
This Pseudo instructions 8080 Assembler: 8080 pseudo instructions pseudo instruction inserts a single or a series of 2-byte words into the code. Words are stored with their least significant byte first. This means, $1234 is stored as $34, $12. Assembler directives: #if, #elif, #else, #endif Pseudo instructions: if, endif If you need them to be stored 'as seen' then use the 'defm' Pseudo instructions 8080 Assembler: 8080 pseudo instructions pseudo instruction. |

[<prev] [top] [next>]