<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="DIL24">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL28">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt;</description>
</package>
<package name="SO-08-150MIL">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
<package name="SO-08M">
<description>&lt;B&gt;Small Outline Medium Plastic Gull Wing&lt;/B&gt;
&lt;p&gt;207-mil body, package type SM 
&lt;br&gt;Microchip SO8 Medium</description>
</package>
<package name="SO-14">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SL</description>
</package>
<package name="DIL8">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
<package name="TSSOP8">
<description>&lt;b&gt;Thin Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type ST</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOJV36-400">
<description>&lt;b&gt;36-Lead (400-Mil) Molded SOJ V36&lt;/b&gt;&lt;p&gt;
Source: CYPRESS cy7c1049cv33_8.pdf</description>
</package>
<package name="TSOPII-44">
<description>&lt;b&gt;44 PIN TSOP II&lt;/b&gt;&lt;br&gt;
18.4 x 10.2mm&lt;br&gt;
pitch 0.8mm&lt;br&gt;
Pad-Abstand von der Mitte: 5.7mm&lt;br&gt;
Pad-Größe: 4.5mm x 1.1mm&lt;br&gt;</description>
</package>
<package name="TSOPII-32">
<description>&lt;b&gt;32-pin TSOP II (51-85095)&lt;/b&gt;&lt;p&gt;
Source: Cypress CYP05780611.pdf</description>
</package>
<package name="SOJ32-400">
<description>&lt;b&gt;32-pin (400-Mil) Molded SOJ (51-85033)&lt;/b&gt;&lt;p&gt;
Source:</description>
</package>
<package name="VFBGA48">
<description>&lt;b&gt;48-ball VFBGA (6 x 8 x 1 mm) (51-85150)&lt;/b&gt;&lt;p&gt;
Source: Cypress CYP05780611.pdf</description>
</package>
<package name="SOJ36-4">
<description>&lt;b&gt;SOJ - Small Outline J-Bend&lt;/b&gt;&lt;br&gt;
w = 400 mils&lt;br&gt;
pitch = 50 mils&lt;br&gt;</description>
</package>
<package name="SOJ44-4">
<description>&lt;b&gt;SOJ - Small Outline J-Bend&lt;/b&gt;&lt;br&gt;
w = 400 mils&lt;br&gt;
pitch = 50 mils&lt;br&gt;</description>
</package>
<package name="SIMM30">
<description>&lt;b&gt;SIMM connector&lt;/b&gt;</description>
</package>
<package name="DIL32">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SIPP30">
</package>
<package name="DIL32-ROUND">
</package>
<package name="DIL32-3">
<description>&lt;B&gt;Dual In Line&lt;/b&gt; 0.3 inch</description>
</package>
<package name="PLCC-S32--SOCKET">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt; Socket</description>
</package>
<package name="PLCC32R">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
rectangle</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="2732">
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="O0" direction="hiz"/>
<pin name="O1" direction="hiz"/>
<pin name="O2" direction="hiz"/>
<pin name="O3" direction="hiz"/>
<pin name="O4" direction="hiz"/>
<pin name="O5" direction="hiz"/>
<pin name="O6" direction="hiz"/>
<pin name="O7" direction="hiz"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE!/VPP" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="2764">
<pin name="VPP" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="O0" direction="hiz"/>
<pin name="O1" direction="hiz"/>
<pin name="O2" direction="hiz"/>
<pin name="O3" direction="hiz"/>
<pin name="O4" direction="hiz"/>
<pin name="O5" direction="hiz"/>
<pin name="O6" direction="hiz"/>
<pin name="O7" direction="hiz"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!PGM" direction="in"/>
</symbol>
<symbol name="27256">
<pin name="VPP" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="O0" direction="hiz"/>
<pin name="O1" direction="hiz"/>
<pin name="O2" direction="hiz"/>
<pin name="O3" direction="hiz"/>
<pin name="O4" direction="hiz"/>
<pin name="O5" direction="hiz"/>
<pin name="O6" direction="hiz"/>
<pin name="O7" direction="hiz"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
</symbol>
<symbol name="27512">
<pin name="A15" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="O0" direction="hiz"/>
<pin name="O1" direction="hiz"/>
<pin name="O2" direction="hiz"/>
<pin name="O3" direction="hiz"/>
<pin name="O4" direction="hiz"/>
<pin name="O5" direction="hiz"/>
<pin name="O6" direction="hiz"/>
<pin name="O7" direction="hiz"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
</symbol>
<symbol name="257">
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="!WR" direction="in"/>
</symbol>
<symbol name="VCC-GND">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="27128">
<pin name="VPP" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="O0" direction="hiz"/>
<pin name="O1" direction="hiz"/>
<pin name="O2" direction="hiz"/>
<pin name="O3" direction="hiz"/>
<pin name="O4" direction="hiz"/>
<pin name="O5" direction="hiz"/>
<pin name="O6" direction="hiz"/>
<pin name="O7" direction="hiz"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="!PGM" direction="in"/>
</symbol>
<symbol name="24AA">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="WP" direction="in"/>
</symbol>
<symbol name="41464">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="I/O1"/>
<pin name="I/O2"/>
<pin name="I/O3"/>
<pin name="I/O4"/>
<pin name="!OE" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="!CAS" direction="in"/>
<pin name="!RAS" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="4MBIT_512KX8">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="I/O00"/>
<pin name="I/O01"/>
<pin name="I/O02"/>
<pin name="I/O03"/>
<pin name="I/O04"/>
<pin name="I/O05"/>
<pin name="I/O06"/>
<pin name="I/O07"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="WE" direction="in" function="dot"/>
<pin name="CE" direction="in" function="dot"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="+3V@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="+3V@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
</symbol>
<symbol name="7C1019">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="I/O00"/>
<pin name="I/O01"/>
<pin name="I/O02"/>
<pin name="I/O03"/>
<pin name="I/O04"/>
<pin name="I/O05"/>
<pin name="I/O06"/>
<pin name="I/O07"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="WE" direction="in" function="dot"/>
<pin name="CE" function="dot"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="+3V@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="+3V@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="61C1024">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!WE" direction="in" function="dot"/>
<pin name="!CE1" direction="in" function="dot"/>
<pin name="!OE" direction="in" function="dot"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CE2" direction="in" function="dot"/>
</symbol>
<symbol name="7C4098">
<pin name="A0" direction="in"/>
<pin name="D0"/>
<pin name="!WE" direction="in" function="dot"/>
<pin name="!CE" direction="in" function="dot"/>
<pin name="!OE" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="!LB" direction="in" function="dot"/>
<pin name="!UB" direction="in" function="dot"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
</symbol>
<symbol name="PWR-2VCC+2GND">
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="S30">
<pin name="!WE" direction="in" function="dot"/>
<pin name="D5"/>
<pin name="A10" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="D4"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="D3"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="D2"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="D1"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D0"/>
<pin name="!CAS" direction="in" function="dot"/>
<pin name="D6"/>
<pin name="A11" direction="in"/>
<pin name="D7"/>
<pin name="Q8" direction="out"/>
<pin name="!RAS" direction="in" function="dot"/>
<pin name="!CAS8" direction="in" function="dot"/>
<pin name="D8" direction="in"/>
</symbol>
<symbol name="FPM-EDO-SIMM30-DRAM">
</symbol>
<symbol name="SRAM-256K*8">
<pin name="!WE" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D0"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
</symbol>
<symbol name="SRAM-681000">
<pin name="!WE" direction="in" function="dot"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D0"/>
<pin name="!CE1" direction="in" function="dot"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in" function="dot"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="CE2" direction="in"/>
</symbol>
<symbol name="DIL32">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
</symbol>
<symbol name="27010">
<pin name="VPP" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="O0" direction="hiz"/>
<pin name="O1" direction="hiz"/>
<pin name="O2" direction="hiz"/>
<pin name="O3" direction="hiz"/>
<pin name="O4" direction="hiz"/>
<pin name="O5" direction="hiz"/>
<pin name="O6" direction="hiz"/>
<pin name="O7" direction="hiz"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!PGM" direction="in"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="28256">
<pin name="!WE" direction="in" function="dot"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="O0" direction="hiz"/>
<pin name="O1" direction="hiz"/>
<pin name="O2" direction="hiz"/>
<pin name="O3" direction="hiz"/>
<pin name="O4" direction="hiz"/>
<pin name="O5" direction="hiz"/>
<pin name="O6" direction="hiz"/>
<pin name="O7" direction="hiz"/>
<pin name="!CE" direction="in" function="dot"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in" function="dot"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
</symbol>
<symbol name="29F040">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="I/O00"/>
<pin name="I/O01"/>
<pin name="I/O02"/>
<pin name="I/O03"/>
<pin name="I/O04"/>
<pin name="I/O05"/>
<pin name="I/O06"/>
<pin name="I/O07"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="WE" direction="in" function="dot"/>
<pin name="CE" direction="in" function="dot"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
</symbol>
<symbol name="AM29F040">
<pin name="!WE" direction="in" function="dot"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="!CE" direction="in" function="dot"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in" function="dot"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
</symbol>
<symbol name="VCC-GND-1">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="4164">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="hiz"/>
<pin name="!WE" direction="in"/>
<pin name="!CAS" direction="in"/>
<pin name="!RAS" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="2732" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2732"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL24">
<connects>
<connect gate="A" pin="!CE" pad="18"/>
<connect gate="A" pin="!OE!/VPP" pad="20"/>
<connect gate="A" pin="A0" pad="8"/>
<connect gate="A" pin="A1" pad="7"/>
<connect gate="A" pin="A10" pad="19"/>
<connect gate="A" pin="A11" pad="21"/>
<connect gate="A" pin="A2" pad="6"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="4"/>
<connect gate="A" pin="A5" pad="3"/>
<connect gate="A" pin="A6" pad="2"/>
<connect gate="A" pin="A7" pad="1"/>
<connect gate="A" pin="A8" pad="23"/>
<connect gate="A" pin="A9" pad="22"/>
<connect gate="A" pin="O0" pad="9"/>
<connect gate="A" pin="O1" pad="10"/>
<connect gate="A" pin="O2" pad="11"/>
<connect gate="A" pin="O3" pad="13"/>
<connect gate="A" pin="O4" pad="14"/>
<connect gate="A" pin="O5" pad="15"/>
<connect gate="A" pin="O6" pad="16"/>
<connect gate="A" pin="O7" pad="17"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2764" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2764"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL28">
<connects>
<connect gate="A" pin="!CE" pad="20"/>
<connect gate="A" pin="!OE" pad="22"/>
<connect gate="A" pin="!PGM" pad="27"/>
<connect gate="A" pin="A0" pad="10"/>
<connect gate="A" pin="A1" pad="9"/>
<connect gate="A" pin="A10" pad="21"/>
<connect gate="A" pin="A11" pad="23"/>
<connect gate="A" pin="A12" pad="2"/>
<connect gate="A" pin="A2" pad="8"/>
<connect gate="A" pin="A3" pad="7"/>
<connect gate="A" pin="A4" pad="6"/>
<connect gate="A" pin="A5" pad="5"/>
<connect gate="A" pin="A6" pad="4"/>
<connect gate="A" pin="A7" pad="3"/>
<connect gate="A" pin="A8" pad="25"/>
<connect gate="A" pin="A9" pad="24"/>
<connect gate="A" pin="O0" pad="11"/>
<connect gate="A" pin="O1" pad="12"/>
<connect gate="A" pin="O2" pad="13"/>
<connect gate="A" pin="O3" pad="15"/>
<connect gate="A" pin="O4" pad="16"/>
<connect gate="A" pin="O5" pad="17"/>
<connect gate="A" pin="O6" pad="18"/>
<connect gate="A" pin="O7" pad="19"/>
<connect gate="A" pin="VPP" pad="1"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27256" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="27256"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL28">
<connects>
<connect gate="A" pin="!CE" pad="20"/>
<connect gate="A" pin="!OE" pad="22"/>
<connect gate="A" pin="A0" pad="10"/>
<connect gate="A" pin="A1" pad="9"/>
<connect gate="A" pin="A10" pad="21"/>
<connect gate="A" pin="A11" pad="23"/>
<connect gate="A" pin="A12" pad="2"/>
<connect gate="A" pin="A13" pad="26"/>
<connect gate="A" pin="A14" pad="27"/>
<connect gate="A" pin="A2" pad="8"/>
<connect gate="A" pin="A3" pad="7"/>
<connect gate="A" pin="A4" pad="6"/>
<connect gate="A" pin="A5" pad="5"/>
<connect gate="A" pin="A6" pad="4"/>
<connect gate="A" pin="A7" pad="3"/>
<connect gate="A" pin="A8" pad="25"/>
<connect gate="A" pin="A9" pad="24"/>
<connect gate="A" pin="O0" pad="11"/>
<connect gate="A" pin="O1" pad="12"/>
<connect gate="A" pin="O2" pad="13"/>
<connect gate="A" pin="O3" pad="15"/>
<connect gate="A" pin="O4" pad="16"/>
<connect gate="A" pin="O5" pad="17"/>
<connect gate="A" pin="O6" pad="18"/>
<connect gate="A" pin="O7" pad="19"/>
<connect gate="A" pin="VPP" pad="1"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27512" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="27512"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL28">
<connects>
<connect gate="A" pin="!CE" pad="20"/>
<connect gate="A" pin="!OE" pad="22"/>
<connect gate="A" pin="A0" pad="10"/>
<connect gate="A" pin="A1" pad="9"/>
<connect gate="A" pin="A10" pad="21"/>
<connect gate="A" pin="A11" pad="23"/>
<connect gate="A" pin="A12" pad="2"/>
<connect gate="A" pin="A13" pad="26"/>
<connect gate="A" pin="A14" pad="27"/>
<connect gate="A" pin="A15" pad="1"/>
<connect gate="A" pin="A2" pad="8"/>
<connect gate="A" pin="A3" pad="7"/>
<connect gate="A" pin="A4" pad="6"/>
<connect gate="A" pin="A5" pad="5"/>
<connect gate="A" pin="A6" pad="4"/>
<connect gate="A" pin="A7" pad="3"/>
<connect gate="A" pin="A8" pad="25"/>
<connect gate="A" pin="A9" pad="24"/>
<connect gate="A" pin="O0" pad="11"/>
<connect gate="A" pin="O1" pad="12"/>
<connect gate="A" pin="O2" pad="13"/>
<connect gate="A" pin="O3" pad="15"/>
<connect gate="A" pin="O4" pad="16"/>
<connect gate="A" pin="O5" pad="17"/>
<connect gate="A" pin="O6" pad="18"/>
<connect gate="A" pin="O7" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC55257DP" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="257"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL28">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WR" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="1"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="18"/>
<connect gate="G$1" pin="D7" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W24257AK" prefix="IC">
<description>32k x 8 Bit 15ns High-Speed SRAM (80386er Cache-RAM)</description>
<gates>
<gate name="G$$1" symbol="257"/>
<gate name="P" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$$1" pin="!CE" pad="20"/>
<connect gate="G$$1" pin="!OE" pad="22"/>
<connect gate="G$$1" pin="!WR" pad="27"/>
<connect gate="G$$1" pin="A0" pad="10"/>
<connect gate="G$$1" pin="A1" pad="9"/>
<connect gate="G$$1" pin="A10" pad="21"/>
<connect gate="G$$1" pin="A11" pad="23"/>
<connect gate="G$$1" pin="A12" pad="2"/>
<connect gate="G$$1" pin="A13" pad="26"/>
<connect gate="G$$1" pin="A14" pad="1"/>
<connect gate="G$$1" pin="A2" pad="8"/>
<connect gate="G$$1" pin="A3" pad="7"/>
<connect gate="G$$1" pin="A4" pad="6"/>
<connect gate="G$$1" pin="A5" pad="5"/>
<connect gate="G$$1" pin="A6" pad="4"/>
<connect gate="G$$1" pin="A7" pad="3"/>
<connect gate="G$$1" pin="A8" pad="25"/>
<connect gate="G$$1" pin="A9" pad="24"/>
<connect gate="G$$1" pin="D0" pad="11"/>
<connect gate="G$$1" pin="D1" pad="12"/>
<connect gate="G$$1" pin="D2" pad="13"/>
<connect gate="G$$1" pin="D3" pad="15"/>
<connect gate="G$$1" pin="D4" pad="16"/>
<connect gate="G$$1" pin="D5" pad="17"/>
<connect gate="G$$1" pin="D6" pad="18"/>
<connect gate="G$$1" pin="D7" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27128" prefix="IC">
<gates>
<gate name="G$1" symbol="27128"/>
<gate name="G$2" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL28">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!PGM" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="O0" pad="11"/>
<connect gate="G$1" pin="O1" pad="12"/>
<connect gate="G$1" pin="O2" pad="13"/>
<connect gate="G$1" pin="O3" pad="15"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="17"/>
<connect gate="G$1" pin="O6" pad="18"/>
<connect gate="G$1" pin="O7" pad="19"/>
<connect gate="G$1" pin="VPP" pad="1"/>
<connect gate="G$2" pin="GND" pad="14"/>
<connect gate="G$2" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24*" prefix="IC">
<description>Serial &lt;B&gt;EEPROM&lt;/B&gt;&lt;p&gt;
I2C</description>
<gates>
<gate name="G$1" symbol="24AA"/>
</gates>
<devices>
<device name="SM" package="SO-08M">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="AA01"/>
<technology name="AA02"/>
<technology name="AA04"/>
<technology name="AA08"/>
<technology name="AA128"/>
<technology name="AA16"/>
<technology name="AA32A"/>
<technology name="C01A"/>
<technology name="C02A"/>
<technology name="C04A"/>
<technology name="C08B"/>
<technology name="C32A"/>
<technology name="C64"/>
<technology name="CL04B"/>
<technology name="LC08B"/>
<technology name="LC128"/>
<technology name="LC16B"/>
<technology name="LC32A"/>
<technology name="LC64"/>
</technologies>
</device>
<device name="SL" package="SO-14">
<connects>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="WP" pad="12"/>
</connects>
<technologies>
<technology name="AA04"/>
<technology name="AA08"/>
<technology name="AA16"/>
<technology name="C01A"/>
<technology name="C02A"/>
<technology name="C04A"/>
<technology name="C08B"/>
<technology name="C16B"/>
<technology name="CL04A"/>
<technology name="LC08B"/>
<technology name="LC16B"/>
</technologies>
</device>
<device name="P" package="DIL8">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="AA01"/>
<technology name="AA02"/>
<technology name="AA04"/>
<technology name="AA08"/>
<technology name="AA128"/>
<technology name="AA16"/>
<technology name="AA256"/>
<technology name="AA32A"/>
<technology name="AA64"/>
<technology name="C01A"/>
<technology name="C02A"/>
<technology name="C04A"/>
<technology name="C08B"/>
<technology name="C16B"/>
<technology name="C32A"/>
<technology name="C64"/>
<technology name="CL04B"/>
<technology name="LC01"/>
<technology name="LC024"/>
<technology name="LC025"/>
<technology name="LC04"/>
<technology name="LC08B"/>
<technology name="LC128"/>
<technology name="LC16B"/>
<technology name="LC256"/>
<technology name="LC32A"/>
<technology name="LC64"/>
<technology name="LCS52"/>
</technologies>
</device>
<device name="SN" package="SO-08">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="AA01"/>
<technology name="AA02"/>
<technology name="AA04"/>
<technology name="AA08"/>
<technology name="AA128"/>
<technology name="AA16"/>
<technology name="AA256"/>
<technology name="AA32A"/>
<technology name="AA64"/>
<technology name="C08B"/>
<technology name="C16B"/>
<technology name="C32A"/>
<technology name="CL04B"/>
<technology name="LC024"/>
<technology name="LC025"/>
<technology name="LC08B"/>
<technology name="LC128"/>
<technology name="LC16B"/>
<technology name="LC256"/>
<technology name="LC32A"/>
<technology name="LC64"/>
<technology name="LCS52"/>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="AA128"/>
<technology name="AA64"/>
<technology name="C64"/>
<technology name="LC024"/>
<technology name="LC025"/>
<technology name="LC128"/>
<technology name="LC64"/>
<technology name="LCS52"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="41464C" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="41464"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="!CAS" pad="16"/>
<connect gate="G$1" pin="!OE" pad="1"/>
<connect gate="G$1" pin="!RAS" pad="5"/>
<connect gate="G$1" pin="!WE" pad="4"/>
<connect gate="G$1" pin="A0" pad="14"/>
<connect gate="G$1" pin="A1" pad="13"/>
<connect gate="G$1" pin="A2" pad="12"/>
<connect gate="G$1" pin="A3" pad="11"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="10"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="I/O1" pad="2"/>
<connect gate="G$1" pin="I/O2" pad="3"/>
<connect gate="G$1" pin="I/O3" pad="15"/>
<connect gate="G$1" pin="I/O4" pad="17"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7C1019CV33" prefix="IC">
<description>&lt;b&gt;128K x 8 Static RAM&lt;/b&gt; 10ns&lt;p&gt;
Source: Cypress CYP05780611.pdf</description>
<gates>
<gate name="G$1" symbol="7C1019"/>
</gates>
<devices>
<device name="ZXC" package="TSOPII-32">
<connects>
<connect gate="G$1" pin="+3V@1" pad="8"/>
<connect gate="G$1" pin="+3V@2" pad="24"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="19"/>
<connect gate="G$1" pin="A11" pad="20"/>
<connect gate="G$1" pin="A12" pad="21"/>
<connect gate="G$1" pin="A13" pad="29"/>
<connect gate="G$1" pin="A14" pad="30"/>
<connect gate="G$1" pin="A15" pad="31"/>
<connect gate="G$1" pin="A16" pad="32"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="14"/>
<connect gate="G$1" pin="A6" pad="15"/>
<connect gate="G$1" pin="A7" pad="16"/>
<connect gate="G$1" pin="A8" pad="17"/>
<connect gate="G$1" pin="A9" pad="18"/>
<connect gate="G$1" pin="CE" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="I/O00" pad="6"/>
<connect gate="G$1" pin="I/O01" pad="7"/>
<connect gate="G$1" pin="I/O02" pad="10"/>
<connect gate="G$1" pin="I/O03" pad="11"/>
<connect gate="G$1" pin="I/O04" pad="22"/>
<connect gate="G$1" pin="I/O05" pad="23"/>
<connect gate="G$1" pin="I/O06" pad="26"/>
<connect gate="G$1" pin="I/O07" pad="27"/>
<connect gate="G$1" pin="OE" pad="28"/>
<connect gate="G$1" pin="WE" pad="12"/>
</connects>
<technologies>
<technology name=""/>
<technology name="-10"/>
<technology name="-12"/>
<technology name="-15"/>
</technologies>
</device>
<device name="VC" package="SOJ32-400">
<connects>
<connect gate="G$1" pin="+3V@1" pad="8"/>
<connect gate="G$1" pin="+3V@2" pad="24"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="19"/>
<connect gate="G$1" pin="A11" pad="20"/>
<connect gate="G$1" pin="A12" pad="21"/>
<connect gate="G$1" pin="A13" pad="29"/>
<connect gate="G$1" pin="A14" pad="30"/>
<connect gate="G$1" pin="A15" pad="31"/>
<connect gate="G$1" pin="A16" pad="32"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="14"/>
<connect gate="G$1" pin="A6" pad="15"/>
<connect gate="G$1" pin="A7" pad="16"/>
<connect gate="G$1" pin="A8" pad="17"/>
<connect gate="G$1" pin="A9" pad="18"/>
<connect gate="G$1" pin="CE" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="I/O00" pad="6"/>
<connect gate="G$1" pin="I/O01" pad="7"/>
<connect gate="G$1" pin="I/O02" pad="10"/>
<connect gate="G$1" pin="I/O03" pad="11"/>
<connect gate="G$1" pin="I/O04" pad="22"/>
<connect gate="G$1" pin="I/O05" pad="23"/>
<connect gate="G$1" pin="I/O06" pad="26"/>
<connect gate="G$1" pin="I/O07" pad="27"/>
<connect gate="G$1" pin="OE" pad="28"/>
<connect gate="G$1" pin="WE" pad="12"/>
</connects>
<technologies>
<technology name="-10"/>
<technology name="-12"/>
<technology name="-15"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="61C1024">
<description>IC61C1024 oder IC61C1024L&lt;br&gt;
High-Speed CMOS Static SRAM (12 .. 25ns)&lt;br&gt;
128K x 8</description>
<gates>
<gate name="G$1" symbol="61C1024"/>
</gates>
<devices>
<device name="SOJ" package="SOJ32-400">
<connects>
<connect gate="G$1" pin="!CE1" pad="22"/>
<connect gate="G$1" pin="!OE" pad="24"/>
<connect gate="G$1" pin="!WE" pad="29"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="3"/>
<connect gate="G$1" pin="A15" pad="31"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="CE2" pad="30"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="17"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="19"/>
<connect gate="G$1" pin="D6" pad="20"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7C4098">
<description>&lt;b&gt;SRAM 256K x 16&lt;/b&gt;&lt;br&gt;
access time: 10 .. 20ns&lt;br&gt;
with lower|upper bank select&lt;br&gt;
7C4098: 5V&lt;br&gt;
7C34098: 3.3V&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="7C4098"/>
<gate name="G$2" symbol="PWR-2VCC+2GND"/>
</gates>
<devices>
<device name="T" package="TSOPII-44">
<connects>
<connect gate="G$1" pin="!CE" pad="6"/>
<connect gate="G$1" pin="!LB" pad="39"/>
<connect gate="G$1" pin="!OE" pad="41"/>
<connect gate="G$1" pin="!UB" pad="40"/>
<connect gate="G$1" pin="!WE" pad="17"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="24"/>
<connect gate="G$1" pin="A12" pad="25"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A15" pad="42"/>
<connect gate="G$1" pin="A16" pad="43"/>
<connect gate="G$1" pin="A17" pad="44"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="18"/>
<connect gate="G$1" pin="A6" pad="19"/>
<connect gate="G$1" pin="A7" pad="20"/>
<connect gate="G$1" pin="A8" pad="21"/>
<connect gate="G$1" pin="A9" pad="22"/>
<connect gate="G$1" pin="D0" pad="7"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="D10" pad="31"/>
<connect gate="G$1" pin="D11" pad="32"/>
<connect gate="G$1" pin="D12" pad="35"/>
<connect gate="G$1" pin="D13" pad="36"/>
<connect gate="G$1" pin="D14" pad="37"/>
<connect gate="G$1" pin="D15" pad="38"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="14"/>
<connect gate="G$1" pin="D6" pad="15"/>
<connect gate="G$1" pin="D7" pad="16"/>
<connect gate="G$1" pin="D8" pad="29"/>
<connect gate="G$1" pin="D9" pad="30"/>
<connect gate="G$2" pin="GND@1" pad="12"/>
<connect gate="G$2" pin="GND@2" pad="34"/>
<connect gate="G$2" pin="VCC@1" pad="11"/>
<connect gate="G$2" pin="VCC@2" pad="33"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J" package="SOJ44-4">
<connects>
<connect gate="G$1" pin="!CE" pad="6"/>
<connect gate="G$1" pin="!LB" pad="39"/>
<connect gate="G$1" pin="!OE" pad="41"/>
<connect gate="G$1" pin="!UB" pad="40"/>
<connect gate="G$1" pin="!WE" pad="17"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="24"/>
<connect gate="G$1" pin="A12" pad="25"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A15" pad="42"/>
<connect gate="G$1" pin="A16" pad="43"/>
<connect gate="G$1" pin="A17" pad="44"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="18"/>
<connect gate="G$1" pin="A6" pad="19"/>
<connect gate="G$1" pin="A7" pad="20"/>
<connect gate="G$1" pin="A8" pad="21"/>
<connect gate="G$1" pin="A9" pad="22"/>
<connect gate="G$1" pin="D0" pad="7"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="D10" pad="31"/>
<connect gate="G$1" pin="D11" pad="32"/>
<connect gate="G$1" pin="D12" pad="35"/>
<connect gate="G$1" pin="D13" pad="36"/>
<connect gate="G$1" pin="D14" pad="37"/>
<connect gate="G$1" pin="D15" pad="38"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="14"/>
<connect gate="G$1" pin="D6" pad="15"/>
<connect gate="G$1" pin="D7" pad="16"/>
<connect gate="G$1" pin="D8" pad="29"/>
<connect gate="G$1" pin="D9" pad="30"/>
<connect gate="G$2" pin="GND@1" pad="12"/>
<connect gate="G$2" pin="GND@2" pad="34"/>
<connect gate="G$2" pin="VCC@1" pad="11"/>
<connect gate="G$2" pin="VCC@2" pad="33"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DUMMY-PWR-2VCC+2GND">
<gates>
<gate name="G$1" symbol="PWR-2VCC+2GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIMM30" prefix="MEM" uservalue="yes">
<description>&lt;b&gt;AMP connector&lt;/b&gt;
&lt;p&gt;30-pin SIMM signle inline memory module for FPM or EDO DRAMs.
&lt;br&gt;8 bit + parity  *  256k, 1M, 4M or 16 M
&lt;p&gt;Address lines are swappable except A9, 10 and 11
&lt;br&gt;Data lines are swappable

&lt;p&gt;Package is original from library</description>
<gates>
<gate name="G$1" symbol="S30"/>
<gate name="G$2" symbol="PWR-2VCC+2GND"/>
</gates>
<devices>
<device name="" package="SIMM30">
<connects>
<connect gate="G$1" pin="!CAS" pad="2"/>
<connect gate="G$1" pin="!CAS8" pad="28"/>
<connect gate="G$1" pin="!RAS" pad="27"/>
<connect gate="G$1" pin="!WE" pad="21"/>
<connect gate="G$1" pin="A0" pad="4"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A10" pad="19"/>
<connect gate="G$1" pin="A11" pad="24"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="11"/>
<connect gate="G$1" pin="A5" pad="12"/>
<connect gate="G$1" pin="A6" pad="14"/>
<connect gate="G$1" pin="A7" pad="15"/>
<connect gate="G$1" pin="A8" pad="17"/>
<connect gate="G$1" pin="A9" pad="18"/>
<connect gate="G$1" pin="D0" pad="3"/>
<connect gate="G$1" pin="D1" pad="6"/>
<connect gate="G$1" pin="D2" pad="10"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="23"/>
<connect gate="G$1" pin="D7" pad="25"/>
<connect gate="G$1" pin="D8" pad="29"/>
<connect gate="G$1" pin="Q8" pad="26"/>
<connect gate="G$2" pin="GND@1" pad="22"/>
<connect gate="G$2" pin="GND@2" pad="9"/>
<connect gate="G$2" pin="VCC@1" pad="1"/>
<connect gate="G$2" pin="VCC@2" pad="30"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SIPP" package="SIPP30">
<connects>
<connect gate="G$1" pin="!CAS" pad="2"/>
<connect gate="G$1" pin="!CAS8" pad="28"/>
<connect gate="G$1" pin="!RAS" pad="27"/>
<connect gate="G$1" pin="!WE" pad="21"/>
<connect gate="G$1" pin="A0" pad="4"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A10" pad="19"/>
<connect gate="G$1" pin="A11" pad="24"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="11"/>
<connect gate="G$1" pin="A5" pad="12"/>
<connect gate="G$1" pin="A6" pad="14"/>
<connect gate="G$1" pin="A7" pad="15"/>
<connect gate="G$1" pin="A8" pad="17"/>
<connect gate="G$1" pin="A9" pad="18"/>
<connect gate="G$1" pin="D0" pad="3"/>
<connect gate="G$1" pin="D1" pad="6"/>
<connect gate="G$1" pin="D2" pad="10"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="23"/>
<connect gate="G$1" pin="D7" pad="25"/>
<connect gate="G$1" pin="D8" pad="29"/>
<connect gate="G$1" pin="Q8" pad="26"/>
<connect gate="G$2" pin="GND@1" pad="22"/>
<connect gate="G$2" pin="GND@2" pad="9"/>
<connect gate="G$2" pin="VCC@1" pad="1"/>
<connect gate="G$2" pin="VCC@2" pad="30"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRAM-681000" prefix="IC">
<gates>
<gate name="G$1" symbol="SRAM-681000"/>
<gate name="PWR" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL32">
<connects>
<connect gate="G$1" pin="!CE1" pad="22"/>
<connect gate="G$1" pin="!OE" pad="24"/>
<connect gate="G$1" pin="!WE" pad="29"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="3"/>
<connect gate="G$1" pin="A15" pad="31"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="CE2" pad="30"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="17"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="19"/>
<connect gate="G$1" pin="D6" pad="20"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="PWR" pin="GND" pad="16"/>
<connect gate="PWR" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27010" prefix="IC" uservalue="yes">
<description>&lt;b&gt;EPROM 128k x 8 bit&lt;/b&gt;

&lt;br&gt;Note: the symbol includes Pin 30 marked as "NC". If this pin is conencted to Vcc then a 27512 EPROM can be inserted into this socket as well.</description>
<gates>
<gate name="A" symbol="27010"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL32">
<connects>
<connect gate="A" pin="!CE" pad="22"/>
<connect gate="A" pin="!OE" pad="24"/>
<connect gate="A" pin="!PGM" pad="31"/>
<connect gate="A" pin="A0" pad="12"/>
<connect gate="A" pin="A1" pad="11"/>
<connect gate="A" pin="A10" pad="23"/>
<connect gate="A" pin="A11" pad="25"/>
<connect gate="A" pin="A12" pad="4"/>
<connect gate="A" pin="A13" pad="28"/>
<connect gate="A" pin="A14" pad="29"/>
<connect gate="A" pin="A15" pad="3"/>
<connect gate="A" pin="A16" pad="2"/>
<connect gate="A" pin="A2" pad="10"/>
<connect gate="A" pin="A3" pad="9"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="A5" pad="7"/>
<connect gate="A" pin="A6" pad="6"/>
<connect gate="A" pin="A7" pad="5"/>
<connect gate="A" pin="A8" pad="27"/>
<connect gate="A" pin="A9" pad="26"/>
<connect gate="A" pin="NC" pad="30"/>
<connect gate="A" pin="O0" pad="13"/>
<connect gate="A" pin="O1" pad="14"/>
<connect gate="A" pin="O2" pad="15"/>
<connect gate="A" pin="O3" pad="17"/>
<connect gate="A" pin="O4" pad="18"/>
<connect gate="A" pin="O5" pad="19"/>
<connect gate="A" pin="O6" pad="20"/>
<connect gate="A" pin="O7" pad="21"/>
<connect gate="A" pin="VPP" pad="1"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="28256">
<description>&lt;b&gt;AT28C256 EEprom&lt;/b&gt;
&lt;br&gt;5V-programmierbar
&lt;br&gt;Programmierbar über Schreibbefehle ~ RAM
&lt;br&gt;weitgehend pinkompatibel zum 27256
&lt;br&gt;28C256: Pin 1 = A14, Pin 27 = !WR
&lt;br&gt;27C256: Pin 1 = Vpp, Pin 27 = A14</description>
<gates>
<gate name="G$1" symbol="28256"/>
<gate name="G$2" symbol="VCC-GND"/>
</gates>
<devices>
<device name="" package="DIL28">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="1"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="O0" pad="11"/>
<connect gate="G$1" pin="O1" pad="12"/>
<connect gate="G$1" pin="O2" pad="13"/>
<connect gate="G$1" pin="O3" pad="15"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="17"/>
<connect gate="G$1" pin="O6" pad="18"/>
<connect gate="G$1" pin="O7" pad="19"/>
<connect gate="G$2" pin="GND" pad="14"/>
<connect gate="G$2" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="29F040" prefix="IC">
<description>4-Megabit &lt;b&gt;FLASH MEMORY&lt;/b&gt;&lt;p&gt;
(512 K x 8 bit) 5 V-only</description>
<gates>
<gate name="G$1" symbol="AM29F040"/>
<gate name="P" symbol="VCC-GND-1"/>
</gates>
<devices>
<device name="-P" package="DIL32-3">
<connects>
<connect gate="G$1" pin="!CE" pad="22"/>
<connect gate="G$1" pin="!OE" pad="24"/>
<connect gate="G$1" pin="!WE" pad="31"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="1"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="17"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="19"/>
<connect gate="G$1" pin="D6" pad="20"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JS" package="PLCC-S32--SOCKET">
<connects>
<connect gate="G$1" pin="!CE" pad="22"/>
<connect gate="G$1" pin="!OE" pad="24"/>
<connect gate="G$1" pin="!WE" pad="31"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="1"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="17"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="19"/>
<connect gate="G$1" pin="D6" pad="20"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-J" package="PLCC32R">
<connects>
<connect gate="G$1" pin="!CE" pad="22"/>
<connect gate="G$1" pin="!OE" pad="24"/>
<connect gate="G$1" pin="!WE" pad="31"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="1"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="17"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="19"/>
<connect gate="G$1" pin="D6" pad="20"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4164">
<gates>
<gate name="G$1" symbol="4164"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="!CAS" pad="15"/>
<connect gate="G$1" pin="!RAS" pad="4"/>
<connect gate="G$1" pin="!WE" pad="3"/>
<connect gate="G$1" pin="A0" pad="5"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="10"/>
<connect gate="G$1" pin="A5" pad="11"/>
<connect gate="G$1" pin="A6" pad="12"/>
<connect gate="G$1" pin="A7" pad="13"/>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="DOUT" pad="14"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
